FreeOCR notes1) For best results set your scanner to 300 DPI , 200 DPI is the minimum setting to achieve acceptable results.2) Use the rotate buttons (to the left of the image) if your image is upside down or rotated3) If your document has columns or pictures then just select the text area by drawing a box on the image with the left mouse button4) After OCR you can use the export button to Word or copy/paste the text into any Windows application.Note: You can press the red X to clear this text window before OCR'ingThis page was prepared using Microsoft Wordprinted then scanned @ 200 DPITimes New Roman"The quick brown fox jumps over a lazy dog""The quick brown fox jumps over a lazy dog""The quick brown fox jumps over a lazy dogArial"The quick brown fox jumps over a lazy dog""The quick brovvn fox jumps over a lazy dog""The quick brown fox jumps over a lazy dog"The phrase above uses all letters from the alphabet.Inn: 91Poloikovy rozpoéetS: 01Horni Bziza-DOZP-stavebni upravy podzemni garézeO: O1Zménovy list 1R: SOD-D1Odpoéet Césti vyméry betonové pfizdivky, odpoéet Césti izo|aoe,odpoéet vykopy vychodniCéstpdpoéet pa2eni,pi‘ipoCet néhrada odtézeného kameniva za zésypovou zeminu, pfipoéetvétéi vyméry asfaltové vrstvy, pﬁpoéet bouréni betonového monumentu,pi‘ipo6et vpustiP.<§.C1slo polozky“ MJ MnoistviNézev polozkyCena I MJCelkemDil: 1Zemni préce136 989,57Dil: 3Svislé a kompletni konstrukce-86 462,1019 311419811R00lzolace perimetndeskami tl.2 cm, nopové féliem2 -27 , 90000164,00-21 315,60-9 s\*3-27.90000| 20 311320050RAOZdi nadzékladové ZB z betonu C 30/37, tl. 15 cmm2-27,900002 335,00-65 146,50-9 3'3-27.90000Dil: 5Komunikace43 427,86Dﬂ: 61Upravy\_povrchl'| vnitini000Dil: 62Upravy\_povrchl‘| vnéj§i-7 477,20Dil: 63Podlahy a podlahové konstrukce0,00Dil: 8Trubni vedeni-6 749,0037 B31350113RAOKanalizaéni pﬁpojka z trub PVC, D 125 mmYT!-4,00000875,0043 500,000pfipo] stévajfci -4—4,00000] 3&2propojeni pfipojky se éachtoukpl-1,000003 249,00-3 249,001pfipo] stévajici —1-1 00000Dil: 91Doplﬁujici préce na komunikaci1 495 00Dil: 93Dokonéovaci préce inistaveb0,00Dil: 96Bouréni konstrukci60 798,03NP2 ‘120901121RT1Bcuréni konstrukci z pf0S1éhO betonu v odkopévkéchpneumatickym kladivemm38,211006 740,0055 342,142,3‘1.7\*2\_18.21100‘NP3 962031113R00Bouréni pﬁéek z cihel pélenych plnych tl. 65 mmm245 , 09000121,005 455,8914'2 75,4\*2,7/Z37.800007.29000Piesun hmot27 237,0652‘979087212R00Naklédéni suti na dopravni prostfedky - komunikace137,46500160,005 994,4011,376-0,271+26 3637.46500| 53 979081111R00Odvoz suti a vybour. hrnot na sklédku do 1 km137,46500172,006 443,9811,376~O 271+26 3637,46500| 54 979081121RO0Pfiplatek k odvozu za kaidy daléi 1 km1187,3250019,003559,1837,465’51873250055 979990102R00Pop|at.za sklédsuti-smés beta cihel137,46500300,0011 239,50Dil: 99Staveni§tni piesun hmot17 708,7959-999281105R00Pfesun hmot pro opravy a Udribu do vyéky 6 m1186,40828,95,0017 708,79181 \_14938+23.12275+1.00205+0.03021-0.46035»127168-171640818640828Dil: 711lzolace proti vodé-28 876,50Dil: 8Trubni vedeni9 700,10NP4 895941311RT2Zfizeni vpusti uliéni z dilcﬁ typ UVB - 50 véetné dodévky kusdilcﬂ pro ulifzni vpusti TBV1,ooooo8 543,608 543,6011,00000|NP5‘B99201111R00Osazeni mfizi litinovych s rémem do 50kgkus1,00000346,50346,50Zpracovéno programem BU|LDpower S, © RTS, a.s. Strénka 1 z 4/11 ,0000OPoloikovy rozpoéetS: {O1 Horni Biiza-DOZP-stavebni upravy podzemni garéieOI ‘O1 Zménovy list1Odpoéet éésti vyméry betonové pﬁzdivky, odpoéet éésti izolaoepdpoéet vykopy vychodnlR: SOD-D1 éést,odpo<':et paieni,pi‘ipo<Eet néhrada odtéieného kameniva za zésypovou zeminu, pfipoéetvétéi vyméry asfaltové vrstvy, pfipoéet bouréni betonového monumentu,p|"ipoéet vpustiP.é. Cislo poloiky Nézev poloiky MJ Mnoistvl Cena I MJ Ce\kemNP6 55242130R Mﬁi vtokové KMA15 300x300x60 mm litina kus 1,0000!) 810,00 810,001 1700000Odpoéty cetkem bez DPH -150 247,43Pfipoéty celkem bez DPH 318 039,04Rozdil 167 791,61Z3 -7 202;} Zpracovéno programem BU|LDpower S, © RTS, as. Strénka 2 z 4