Příloha č. 1 ‐ Přesná specifikace požadované konfigurace

HW ‐ server Lenovo SR630 (část 1.)

Tato část bude dodána do lokality Horoměřická na adresu Horoměřická 2307, 16400 Praha 6 – Dejvice

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| AUW0 | ThinkSystem SR630 2.5" Chassis with 8 Bays | 1 |
| B5S1 | Intel Xeon Gold 5222 4C 105W 3.8GHz Processor | 1 |
| B4H4 | ThinkSystem 64GB TruDDR4 2933MHz (2Rx4 1.2V) RDIMM | 8 |
| AUWB | ThinkSystem SR530/SR630/SR570 2.5" SATA/SAS 8‐Bay Backplane | 1 |
| 5977 | Select Storage devices ‐ no configured RAID required | 1 |
| B4RQ | ThinkSystem RAID 730‐8i 2GB Flash PCIe 12Gb Adapter | 1 |
| B6TL | ThinkSystem 2.5" PM1643 960GB Entry SAS 12Gb Hot Swap SSD | 2 |
| AUWC | ThinkSystem SR530/SR570/SR630 x8/x16 PCIe LP+LP Riser 1 Kit | 1 |
| AUWQ | Lenovo ThinkSystem 1U LP+LP BF Riser Bracket | 1 |
| AUKH | ThinkSystem 1Gb 4‐port RJ45 LOM | 1 |
| ATZC | QLogic 16Gb Enhanced Gen5 FC Dual‐port HBA | 1 |
| ATPX | Intel X550‐T2 Dual Port 10GBase‐T Adapter | 1 |
| AVWA | ThinkSystem 750W (230/115V) Platinum Hot‐Swap Power Supply | 2 |
| 6400 | 2.8m, 13A/100‐250V, C13 to C14 Jumper Cord | 2 |
| AUPW | ThinkSystem XClarity Controller Standard to Enterprise Upgrade | 1 |
| AXCA | ThinkSystem Toolless Slide Rail | 1 |
| B0MJ | Feature Enable TPM 1.2 | 1 |
| B7XZ | Disable IPMI‐over‐LAN | 1 |
| AWGE | ThinkSystem SR630 WW Lenovo LPK | 1 |
| BCH1 | ERP LOT9 Solution Country | 1 |
| AUWX | 8x2.5" HDD BP Cable Kit | 1 |
| B0ML | Feature Enable TPM on MB | 1 |
| AVEN | ThinkSystem 1x1 2.5" HDD Filler | 6 |
| AUWK | Lenovo ThinkSystem 4056 Fan Dummy | 1 |
| AUS6 | Lenovo ThinkSystem 1U height CPU HS Dummy | 1 |
| AUWL | Lenovo ThinkSystem 1U LP Riser Dummy | 1 |
| AURR | ThinkSystem M3.5 Screw for Riser 2x2pcs and Planar 5pcs | 2 |
| AUX0 | ThinkSystem Package for SR630 | 1 |
| AVWJ | ThinkSystem 750W Platinum RDN PSU Caution Label | 1 |
| AUTV | ThinkSystem large Label for non‐24x2.5"/12x3.5"/10x2.5" | 1 |
| B173 | Companion Part for XClarity Controller Standard to Enterprise Upgrade in Factory | 1 |
| AULP | ThinkSystem 1U CPU Heatsink | 1 |
| AUWG | Lenovo ThinkSystem 1U VGA Filler | 1 |
| AVJ2 | ThinkSystem 4R CPU HS Clip | 1 |
| B4NK | ThinkSystem SR630 Refresh MB | 1 |
| AURN | Lenovo ThinkSystem Super Cap Box | 1 |
| AUTJ | ThinkSystem common Intel Label | 1 |
| AUX4 | MS 1U Service Label LI | 1 |
| AUX3 | ThinkSystem SR630 Model Number Label | 1 |
| AVWK | ThinkSystem EIA Plate with Lenovo Logo | 1 |
| AWF9 | ThinkSystem Response time Service Label LI | 1 |
| B6ZL | ThinkSystem SR630 Agency Label Lenovo, No ES Mark | 1 |
| AUTA | XCC Network Access Label | 1 |
| B4X6 | SuperCap for Raid 730‐8i 2GB | 1 |
| 5PS7A01504 | Essential Service ‐ 3Yr 24x7 4Hr Resp + YDYD SR630 | 1 |

HW ‐ server Lenovo Flex SN550 (část 2.)

Tato část bude dodána do sídla zadavatele na adresu Vyšehradská 57, 128 00 Praha 2

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| B4KB | Lenovo ThinkSystem SN550 CLX Server | 1 |
| B5S1 | Intel Xeon Gold 5222 4C 105W 3.8GHz Processor | 2 |
| B4H4 | ThinkSystem 64GB TruDDR4 2933MHz (2Rx4 1.2V) RDIMM | 8 |
| AUYS | ThinkSystem RAID 930‐4i‐2GB 2 Drive Adapter Kit for SN550 | 1 |
| 5977 | Select Storage devices ‐ no configured RAID required | 1 |
| B4Y4 | ThinkSystem 2.5" SS530 400GB Performance SAS 12Gb Hot Swap SSD | 2 |
| AUYN | ThinkSystem SN550/SN850 Fabric Connector | 1 |
| AVCW | ThinkSystem Emulex LPm16002B‐L Mezz 16Gb 2‐Port Fibre Channel Adapter | 1 |
| B0MJ | Feature Enable TPM 1.2 | 1 |
| B7XZ | Disable IPMI‐over‐LAN | 1 |
| AV2Q | Lenovo ThinkSystem SN550 Server WW packaging ‐ Standard | 1 |
| AUXY | Lenovo ThinkSystem Server HDD Bezel Facia | 1 |
| AVUN | Lenovo ThinkSystem SN550 Server Service Label LI | 1 |
| B6VR | ThinkSystem SN550 Agency Label without Energy Star | 1 |
| AULQ | ThinkSystem 1U CPU Performance Heatsink | 1 |
| AVJ2 | ThinkSystem 4R CPU HS Clip | 2 |
| AUY0 | Lenovo ThinkSystem SN550 Server Cover | 1 |
| AUY3 | Lenovo ThinkSystem SN550 Server Air Baffle | 1 |
| AV2U | Lenovo ThinkSystem Server Rear CPU Heatsink | 1 |
| AXHD | Intel Inside Xeon Label | 1 |
| B0ML | Feature Enable TPM on MB | 1 |
| AV2S | System Documentation | 1 |
| 5PS7A01902 | Essential Service ‐ 3Yr 24x7 4Hr Resp + YDYD SN550 | 1 |

HW/SW ‐ řídící storage jednotka (část 3.)

Tato část bude z jedné poloviny (tj. vždy 1/2 kusů uvedených ve sloupci C ke každému produktu) dodána do sídla zadavatele na adresu Vyšehradská 57, 128 00 Praha 2

Tato část bude z jedné poloviny (tj. vždy 1/2 kusů uvedených ve sloupci C ke každému produktu) dodána do lokality Horoměřická na adresu Horoměřická 2307, 16400 Praha 6 – Dejvice

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| 2072‐2H4 | FlashSystem 5010 SFF Control Enclosure | 2 |
| 9730 | Power Cord ‐ PDU Connection | 2 |
| ACSQ | 1m OM3 Fiber Cable (LC) | 8 |
| ACSR | 5m OM3 Fiber Cable (LC) | 8 |
| ADN1 | Order Type 1 ‐ CTO | 2 |
| AG00 | Shipping and Handling NC | 2 |
| AHPA | AC Power Supply HE | 2 |
| AHZE | Hybrid Flash Indicator | 2 |
| AL6B | 2.4TB 10K 2.5 Inch HDD | 28 |
| AL81 | 3.84TB 12 Gb SAS 2.5 Inch Flash Drive | 20 |
| ALBB | 16Gb FC Adapter Pair | 2 |
| ALE7 | FlashCopy Upgrade | 2 |
| ALE8 | Remote Mirroring | 2 |
| ALE9 | Easy Tier | 2 |
| ALGA | Storwize V5000E Cache Upgrade | 2 |