Příloha č. 1 - Přesná specifikace požadované konfigurace

Výzvy Upgrade HW výpočetních a kapacitních zdrojů pro lokalitu Jehněčí dvůr ZAK 20-0342

HW - Serverová skříň RACK (část 1.)

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| 93614PX | Lenovo 42U 1200mm Deep Static Rack | 1 |
| 00YJ778 | 0U 21 C13/12 C19 32A 3 Phase PDU | 2 |

HW - expanzní jednotka storage (část 2.)

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| 2078-12G | FlashSystem 5100 LFF Expansion Enclosure | 1 |
| 9730 | Power Cord - PDU Connection | 1 |
| AC3E | 14TB 7.2K 3.5 Inch NL HDD | 12 |
| ACUA | 0.6m 12Gb SAS Cable(mSAS HD) | 2 |
| ADN1 | Order Type 1 - CTO | 1 |
| AG00 | Shipping and Handling NC | 1 |
| AHPA | AC Power Supply HE | 1 |
| AHZE | Hybrid Flash Indicator | 1 |

HW - pásková knihovna s příslušenstvím (část 3.)

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| 3555-L3A | TS4300 Tape Library | 1 |
| 1411 | Fibre tape drive support | 1 |
| 1682 | Path Failover | 1 |
| 1900 | Additional Power Supply | 1 |
| 7002 | Rack Mount Kit | 1 |
| 8002 | LTO Cleaning Cartridge | 3 |
| 8806 | Ultrium 8 Data Cartridge (5-Pack) | 7 |
| 9212 | Attached to Windows System | 1 |
| 9213 | Attached to Other Non-IBM Systems | 1 |
| 9215 | Attached to Linux System | 1 |
| 9400 | Attached to i5/OS or OS/400 System | 1 |
| 9600 | Attached to IBM AIX System | 1 |
| 9848 | Rack to PDU line cord | 1 |
| AG00 | Shipping and Handling NC | 1 |
| AGK1 | 10 meter OM3 fiber Cable (LC) | 3 |
| AGKM | LTO 8 HH Fibre channel drive | 3 |

Příslušenství současné páskové páskové knihovny (část 4.)

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| 3589-004 | Ultrium cleaning cartridges | 1 |
| 8B3635 | Single LTO cleaner cartridge | 3 |
| 3589-551 | 6 TB Ultrium 7 Tape Cartridge 20-pack Labeled | 1 |
| 5501 | 6 TB Labeled 20-pack | 1 |
| 9022 | Color/vibrant background | 1 |
| 9100 | First character of Volser is 0 | 1 |
| 9200 | Second character of Volser is 0 | 1 |
| 9300 | Third character of Volser is 0 | 1 |

|  |  |  |
| --- | --- | --- |
| 9400 | Fourth character of Volser is 0 | 1 |
| 9500 | Fifth character of Volser is 0 | 1 |
| 9600 | Sixth character of Volser is 0 | 1 |
| 9910 | Base 10 Count LBL Sequence | 1 |

SW - expanzní jednotka storage (část 5.)

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| 5639-SSL | SPECTRUM VIRTUALIZE SOFTWARE FOR STORWIZ | 1 |
| 9000 | BASE PER STORAGE DEVICE SW MAINT 3 YEAR | 1 |
| UCX3C5 | IBM SPECTRUM VIRTUALIZE SOFTWARE FOR STO | 1 |
| 5639-SV8 | IBM Spectrum Virtualize Software for Storwize V50x0 Expansion V8 | 1 |
| UDMUC1 | IBM V50x0 Expansion Base SW with 1 Year SW Maintenance, Per Storage Device | 1 |