ARCTIK^ -io/-30°c
LABORATORY FREEZER
true cooling specialists

LF 500
HIGH LEVEL OF SECURITY FOR YOUR SAMPLES, DUE TO THE GREAT
COOLING PERFORMANCE WITH AIR FORCED COOLING. Automatic defrost
saves you time to focus on what's most important and stores the samples safely.

STAINLESS STEEL		FLEXIBLE STORAGE		GREAT COOLING	
& SPARK FREE		SOLUTIONS		PERFORMANCE	
The unit is available with stainless steel		Arctiko’s LF range is a highly		Air forced cooling provides superior	
AISI 304 Exterior, so that the interior		customizable allowing you to choose		temperature uniformity and stability.	
and exterior is made entirely of stainless		between a wide range of universal		Forcing the airflow around the shelves	
steel, providing a stronger more resistant		shelves and drawers.		and the stored items, ensures that all	
unit.				parts of the unit is equally cold and	
		This allows the user to organize their		avoids any cold or hot spots. Distributed	
This unit can be made in an ATEX version		unit exactly as desired. Our universal		by a powerful fan and open air flow	
- approved according to EN 60079-15		shelf and drawer guides allow you to mix		areas along the sides, the air is always	
category 3, zone 2. CE EX 11-/3 G		shelves and drawers for flexible storage		distributed evenly throughout the fully	
				loaded unit.	
MAIN DIMENSION FOR LF 500		
620

860
	
	-T	
l	631	
	■ j	
O
in
m	t
l	
	■	
I	[	
A-A
o
o

435

650

<v
MAIN SPECIFICATIONS
Item code	DAI 0245 / DAI 0246	
Temperature range (°C)	-10/-30	
Max. ambient temperature (*C)	25	
Capacity (L)	515	
Exterior dimensions WxDxH (mm)	620x860x1997	
Interior dimensions WxDxH (mm)	500x685x1505	
Weight (KG)	130	
Insulation (mm)	60	
Cooling technology	air forced	
Controller model / probe type	G214 / PT1000	
POWER
Power supply (V)	230*	
Frequency (Hz)	50/60	
Power consumption (kWh/24H)	9,6	
AMP (A)	4.2	
Power (Watt)	577	
Horse power (HP)	3/4	
ALARM FUNCTIONS
Alarm display as text - not codes	yes	
Visual / acoustic alarm	yes / yes	
Power failure alarm	yes	
Adjustable high / low temperature alarm	yes / yes	
Open door alarm	yes	
Probe failure alarm	yes	
Low battery alarm	yes	
Compressor failure alarm	no	
Battery backup for alarms (approx, hrs.)	72	
DATA LOGGING & EXTERNAL CONNECTION
Voltage free contact for remote alarm (e.g. GSM alarm module)	yes	
Electronic data logger	yes	
RS 485 port	yes	
USB port for software update & data download	yes	
Temperature chart recorder	optional	
DISPLAY FEATURES	
OPTIONAL
ACCESSORIES
GSM alarm module Temperature chart recorder Shelves (perforated, wire plastic coated, wire stainless steel) Drawers (stainless steel)
Modbus adapter Voltage stabilizer Voltage converters LED light
#
OTHER FEATURES
Automatic defrost	yes	
Antifreeze function	no	
Vacuum release port	no	
Access port for external probe etc. (int. diameter mm)	12	
Light	no	
Lock with key	yes	
Castors (total pcs) / castors with brake (pcs)	4/2	
Fixed feet (pcs) / levelling feet (pcs)	no	
Sub lids / inner doors (pcs)	no	
Reversible door(s)	yes	
Fixed shelves (pcs) / adjustable shelves (pcs)	0/3	
Max. no. of shelves (pcs) / recommended max. no. of shelves (pcs)	23/11	
Max. load per shelf (kg)	30	
Adjustable drawers (pcs)	optional	
Max. no. of adjustable drawers (pcs)	8	
Max. load per adjustable drawer (kg)	30	
TRIGON PLUS
Západní 93. 251 01 Čestfice
Tel.: *420 272 680 190
Email: mail@trigonplus.cz web: www.trigonplus.cz
Number of compressors	1	
Refrigerant	R290	
Interior cabinet material	stainless steel	
Exterior cabinet material	painted steel / stainless steel	
Colour (exterior cabinet)	white / stainless steel	
Foam type	polyurethane	
VIP vacuum insulated panels	no	
SHIPPING	
Shipping weight (KG)	184	
Shipping dimensions WxDxH (cm)	101x74x220	
Shipping volume (m3)	1,64	
\\Vfr-v vT r
110V/60Hz available as option
Display type	4,3" with touch buttons	
Number of optional reference probes	2	
Password protection for turning unit on / off	yes	
Temperature graph on display	yes	
	A©		
Arctiko A/S			
Oddesundvej 39 DK-S715 Esbjerg N Phone: r45 7020 0328	C r W		
infoiftarctiko.com	arctiko.com		**nricatP	"j	

Nabídka

®
.řešeni pro vaši laboratoř
Číslo dokladu:	NA21011796
Garant:	Jonáš Jarník
Datum:	18.01.2021
Datum platnosti:	04.03.2021
Dodavatel:
TRIGON PLUS s.r.o.
Západní 93 251 01 Čestlice
Sídlo: Západní 93, 251 01 Čestlice
IČ: 46350110, DIČ: CZ46350110 Spisová značka v OR Praha: C11127 tel: 272680190, fax: 272680914 e-mail: mail@trigonplus.cz Internet: www.trigonplus.cz
Platební údaje:
Způsob úhrady:	Bankovním převodem
Měna:	CZK
Mrazicí box -10°C až -30°C LF 500, objem 5151
Odběratel:
Nemocnice s poliklinikou Havířov, příspěvková organizace

Dělnická 1132/24
736 01 Havířov - Město
Sídlo: Dělnická 1132/24, 736 01 Havířov
IČ: 00844896, DIČ: CZ00844896 tel: 731672211

Obchodní údaje:
Doprava:
Katalog, číslo Název- popis	Ks	Cenaza jedn. Cena bez DPH DPH Cena s DPH
DAI0245	LF 500, mrazící skříňový box -10/-30°C	1	96 000,00	96 000,00	21%	116 160,00
kapacita 515 litrů
teplota nastavitelná v rozsahu -10°C až -30°C nucená cirkulace vzduchu zaměnitelné umístěni dveří
mikroprocesorové řízeni - ovládači panel s displejem řídicí jednotka s funkci datalogger zálohovaná akumulátorem výstup dat přes RS 232/485 nebo USB
optické a akustické alarmy (vysoká / nízká teplota, výpadek proudu, otevřené dveře, teplotní čidlo)
kontakt pro dálkový přenos alarmu
vnější plášť bílý, odolný čistícím a desinfekčním roztokům
vnitřní komora z nerezu
3 ks stavitelných polic součásti dodávky
příprava pro instalaci nezávislého čidla
automatické odmrazováni
uzamykatelné dveře
přistroj umistěn na 4 kolečkách pro snadnou manipulaci
chladivo R404a
vnější rozměry (šxh x v):
620 x 860 x 1997 mm váha 132 kg
S5200137	Vstupní validace mrazicího/chladicího boxu do - 80°C, 3 měřicí místa, vystavení protokolu, kontrola - ZDARMA	1	0,00	0,00	21%	0,00	
S5200149	doprava nákladní do 3,5t	1	0,00	0,00	21%	0,00	
S5200147	instalace	3	0,00	0,00	21%	0,00	
kalkulace po 1. hodině, dále každých započatých 30 min
součástí je stěhování v rámci bezbariérového přístupu, stěhování mimo bezbariérovou cestu není součástí, volitelně podle velikosti a podmínek od:
S55601	transport do 200 kg
volitelně záznam a alarm	0	4 470,00	0,00	21%	0,00	
TU0843M	záznamník teploty a GSM komunikátor, 2x vstup Pt1000 + 2x dvoustavový vstup	0	12 310,00	0,00	21%	0,00	
GSM datalogger je určen pro záznam teploty ze dvou externích sond a dvou dvoustavových vstupů.
V případě překročení nastavených mezi umožňuje zasíláni alarmových SMS a JSON zpráv přes GPRS datové pnpojení.
Vystavil:
software Áltuš VAŘIO-www.vario.cz~
Stránka 1 z 2
pokračování na straně 2

Nabídka

řešeni pro vaší laboratoř
Katalog, číslo Název - popis	Ks Cena za jedn. Cena bez DPH DPH
Měřené hodnoty mohou být zasílány do internetového úložiště COMET Cloud, což je kompletní monitorovací, alarmovaci a analytický systém.
Nebo je možné nastavit pravidelné zasíláni JSON zpráv do programu COMET Database, interval zasíláni je nastavitelný.
Alarmy jsou rovněž indikovány lokálně na přístroji pomocí LED, LCD a akusticky.
Záznam je prováděn do energeticky nezávislé elektronické paměti.
Údaje lze kdykoli přenést dodaným kabelem do osobního počítače přes rozhraní USB-C.
Celkem:
SIM kartu zajišťuje uživatel.
»> Trigon plus - akreditovaná kalibrační laboratoř
L 2377 - kalibrace měřidel teploty «<
Kalibrace měřidel teploty, jedno a více bodové měřeni teploty v zařízeních s regulaci teploty
ve stálých i mimo stálé prostory laboratoře.
Celkem bez DPH Celkem DPH 8 mj 96 000,00	20 160,00
Cena již obsahuje dopravu, instalaci a školení. Termín dodání aktuálně polovina února 2021. Záruka: 2 roky, servis a validace TRIGON PLUS, pobočka Brno, Praha
Vystavil:
Cena s DPH
Celkem s DPH 116160,00
software Altus VArIÓ - www.vano.cz
Stránka 2 z 2