|  |  |
| --- | --- |
|   |  |
| **IBM FlashSystem 5200 NVMe Control Enclosure** |  |
| **P/N** | **popis** | **ks** |
| 4662-6H2 | IBM FlashSystem 5200 NVMe Control Enclosure | 1 |
|   |   |   |
| 9730 | Power Cord - PDU Connection | 1 |
| ADN1 | Order Type 1 Indicator - CTO | 1 |
| AG00 | Shipping and Handling - No Charge | 1 |
| AGS6 | 9.6 TB NVMe Flash Core Module | 8 |
| AHPE | AC Power Supply (Pair) | 1 |
| AHZD | All Flash Solution Indicator | 1 |
| ALBJ | 16 Gb FC 4 Port Adapter Cards (Pair) | 1 |
| ALG0 | 64 GB Base Cache | 1 |
| ALGC | 192 GB Cache Upgrade | 1 |
| ALH0 | Expert Care Indicator | 1 |
| ALJ3 | EC Basic 3 Year | 1 |
|   |   |   |
| 4663-B03 | 3 year Expert Care Basic for FS5200 | 1 |
|  |  |  |
|  |  |  |
| **IBM FlashSystem 5015 SFF Control Enclosure** |  |
| **P/N** | **popis** | **ks** |
| 2072-2N4 | IBM FlashSystem 5015 SFF Control Enclosure | 1 |
|   |   |   |
| 8S1852 | FS5000 FlashCopy Promo - FC ALE7 | 1 |
| 8S1853 | FS5000 Remote Mirroring Promo - FC ALE8 | 1 |
| 8S1854 | FS5000 EasyTier Promo - FC ALE9 | 1 |
| 9730 | Power Cord - PDU Connection | 1 |
| ADN1 | Order Type 1 - CTO | 1 |
| AG00 | Shipping and Handling NC | 1 |
| AHPA | AC Power Supply HE | 1 |
| AHZE | Hybrid Flash Indicator | 1 |
| AL81 | 3.84TB 12 Gb SAS 2.5 Inch Flash Drive | 8 |
| ALBB | 16Gb FC Adapter Pair | 1 |
| ALGA | Storwize V5000E Cache Upgrade | 1 |