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ENCLOSURE 2

PURCHASER’S MINIMUM REQUIREMENTS FOR PREVENTIVE MAINTENANCE OF THE WORK


	









The terms specified in this Enclosure 2 to the CONTRACT in capital letters, which are not expressly defined in this Enclosure 2, have the meaning assigned to them in the CONTRACT.

The Client stipulates the following minimum requirements for PREVENTIVE MAINTENANCE OF THE WORK:

1) [bookmark: _Ref522012903]Purpose of PREVENTIVE MAINTENANCE
PREVENTIVE MAINTENANCE must be directed towards reducing the probability of a fault in the WORK or limitation of availability of the WORK. Furthermore, PREVENTIVE MAINTENANCE must be directed towards ensuring the operability, reliability, safety and quality of the WORK;

2) Minimum periodicity of PREVENTIVE MAINTENANCE
The CONTRACTOR must perform PREVENTIVE MAINTENANCE OF THE WORK at such a frequency to maintain the purpose of PREVENTIVE MAINTENANCE pursuant to clause 1) of this Enclosure 2 to the CONTRACT, but always at least once (1) every three (3) MONTHS. Within the first year after the signing the PROVISIONAL ACCEPTANCE CERTIFICATE of the WORK by the PURCHASER, the CONTRACTOR must perform PREVENTIVE MAINTENANCE three times (3x) without delay no later than fourteen (14) DAYS, after:
· three (3) MONTHS from the date of signing the PROVISIONAL ACCEPTANCE CERTIFICATE of the WORK;
· six (6) MONTHS from the date of signing the PROVISIONAL ACCEPTANCE CERTIFICATE of the WORK; and
· twelve (12) MONTHS from the date of signing the PROVISIONAL ACCEPTANCE CERTIFICATE of the WORK.
If Enclosure 13 to the Contract states that the CONTRACTOR shall perform PREVENTIVE MAINTENANCE more than once (1) every three (3) MONTHS, the CONTRACTOR is obliged to maintain this higher frequency of PREVENTIVE MAINTENANCE specified in Enclosure 13 to the CONTRACT.

3) Minimum content of PREVENTIVE MAINTENANCE
PREVENTIVE MAINTENANCE must, among others, include the performance of specific inspections of the WORK, removal of identified defects in the WORK, replacement of fast-wearing parts, assessment of operation of the WORK, identification of risks related to operation of the WORK and information about potential improvements to operation of the WORK.
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