
**Ultrazvuková vodní lázeň**

**Typ: SONOREX Digitec DT 31 H**

- 4-step operation as "plug and clean"  
- Timer with countdown and continuous operation  
- Degas - Freely selectable pulse sound - visible on the LED display  
- Stainless steel case against spray, degree of protection IP 33  
- SweepTec for permanent sound field  
- Heating  
  
dimensions:  
Internal tank: 190 x 85 x 60 Outside: 205 x 100 x 170 mm LxWxH  
Content: 0.9 liters  
Filling volume 0.6 liters  
  
Packaging: 320 × 235 × 190 mm, L × W × H  
  
Features: Internal tank: Stainless steel 1.4301  
Housing stainless steel 1.4301  
against spray  
Degree of protection: IP 33  
Timer: 1, 2, 3, 4, 5, 10, 15, 30 min and 8  
Heating 65 ° C fixed 70 Watt  
  
Technical specifications:  
Transducers: 1 PZT broad beam transducers System  
HF generator: overload protected, constant power  
Modes: Easy half-wave  
Operating frequency: 35 kHz, automatic frequency control  
Ultrasonic peak output: 240 W \*  
RF power: 30 watts rms  
Current consumption: - 0.2 A  
Power supply: 230 V ~ 50/60 Hz  
Leakage current: <0.5 mA  
Power cable: fixed to the device, 2 meters long  
  
**Koš K 08** stainless steel  
170 x 65 x 50 mm, mesh size 4 x 4   
  
**Víko D 08**  
stainless steel