|  |  |
| --- | --- |
| **ks** | **Název** |
| 1 | DELL PowerEdge R360 |
| 1 | PowerEdge R360 Server |
| 1 | Trusted Platform Module 2.0 V3 |
| 1 | 2.5" Chassis with up to 8 Hot Plug Hard Drives, Front PERC |
| 1 | Intel Xeon E-2434 3.4G, 4C/8T, 12M Cache, Turbo, HT (55W) DDR5 |
| 1 | Heatsink |
| 1 | Performance Optimized |
| 1 | 5600MT/s UDIMMs |
| 2 | 32GB UDIMM, 5600MT/s ECC |
| 1 | Unconfigured RAID |
| 1 | PERC H355 Controller Front |
| 1 | Front PERC Mechanical Parts, front load |
| 4 | 480GB SSD SATA Read Intensive 6Gbps 512 2.5in Hot-plug AG Drive, 1 DWPD |
| 2 | 2.4TB Hard Drive SAS FIPS-140 10K 512e 2.5in Hot-Plug |
| 1 | Power Saving BIOS Settings |
| 1 | No Energy Star |
| 1 | No Additional FAN for 3.5" Chassis |
| 1 | Dual, (1+1)RDNT, Hot-Plug PSU, 700W MM HLAC (200-240V ONLY, not for 100-120V outlet) Titanium |
| 2 | C13 to C14, PDU Style, 10 AMP, 6.5 Feet (2m), Power Cord |
| 1 | Riser Config 0, No Riser |
| 1 | PowerEdge R360 Motherboard with with Broadcom 5720 Dual Port 1Gb On-Board LOM |
| 1 | PowerEdge 1U Standard Bezel |
| 1 | Dell Luggage Tag R360 |
| 1 | BOSS Blank |
| 1 | iDRAC9, Enterprise 16G |
| 1 | Dell Connectivity Client - Enabled |
| 1 | Dell Connectivity Module |
| 1 | iDRAC,Factory Generated Password, No OMQR |
| 1 | iDRAC Service Module (ISM), NOT Installed |
| 1 | iDRAC Group Manager, Disabled |
| 1 | ReadyRails Sliding Rails Without Cable Management Arm (A12) |
| 1 | PowerEdge R360 Shipping EMEA1 (English/French/German/Spanish/Russian/Hebrew) |
| 1 | PowerEdge R350/R360 Shipping Material for 2.5" Chassis |
| 1 | PowerEdge R360 CE and CCC Marking |
| 1 | Titanium PSU configuration |
| 1 | UEFI BIOS Boot Mode with GPT Partition |
| 1 | No Operating System |
| 1 | No Media Required |
| 1 | No Systems Documentation, No OpenManage DVD Kit |
| 1 | Basic Next Business Day 12 Months |
| 1 | ProSupport and Next Business Day Onsite Service Initial, 12 Month(s) |
| 1 | ProSupport and Next Business Day Onsite Service Extension, 24 Month(s) |