IČO: 48582972 DIČ: CZ48582972
Uni-Export Instruments, s.r.o.

	Šultysova 642/15
Břevnov
169 00 Praha

Objednatel:

Dodavatel:

	IČO: 67985858 
	DIČ: CZ67985858
	Ústav chemických procesů AV ČR, v. v. i.
	
	Rozvojová 135/1
Lysolaje 
165 00 Praha

Datum vystavení: 	09.04.2026
Datum dodání:	15.05.2026
Forma dopravy:		prodejce

Konečný příjemce:
	Kordač Petronilho Orvalho Sandra Cristina, Ph.D.

	 

.
.
Nabídka dodavatele ze dne 15.01.2026, číslo: IC/6137, p. ing. M. Černík.
.
.

Množství	MJ	Název položky	Částka celkem	
1	ks	31874AD3221

Software ADVANCE| DropShape - Contact
Angle Moduleto determine static and
dynamic contact angles using sessile
drop and captive bubble methods.To
control camera, illumination,
temperature, dosing modules, table
movements (depending on modules
selected), to measure, store and report
measured contact angle values.Supported
models: Conic Section, Polynom, Circle,
Young-Laplace, Height WidthMeasuring
range: 0-180°Resolution: 0.01°
.
 	97 405,00	
1	ks	37756AD62

Software ADVANCE | Surface Free Energy
Moduleto determine surface free energy
of solids from contact angle data.The
surface free energy splits into its
polar and dispersive components, its
acid and base components as well as its
hydrogen bonding components, according
to different models.The software
calculates wetting envelope.
.
 	150 040,00	
1	ks	31876AD3223

Software ADVANCE | DropShape - Surface
and Interfacial Tension Module Ito
determine surface and interfacial
tension of liquids by analysis of
pendant drop and rising drop as well as
determination of E' and E'' using the
oscillating drop method.(depending on
modules selected)Supported model:
Young-LaplaceMeasuring range: 0.01-2000
mN/mResolution: 0.01 mN/m.
.
 	150 040,00	
1	ks	39683DS4270

Piezo-driven Oscillating Drop
ModuleModule to characterize the
rheological properties at interfaces,
with integrated temperature control of
the syringe volume.Temperature range: -
10°C - 70°C (263 - 343 K)Fluid tempered.
Permitted fluids: Water, Julabo
H10consisting of:· DO3270 Piezo-driven
ODM dosing unit Hardware for Oscillating
Drop Method· NM3202 Needle mover with
fine positioning· Power supply· TP20
Temperature Probe Pt100 (1/3 DIN B ±
0.1°C)· SY70 500 µl-Glass syringe for
DO3270· SC01 Glass Cuvette with top
cover, 24x24x26 mm· 10 needles for
dosing
FM4200 is required.
Software module AD3223/AD3225 is
required.
.
 	384 780,00	
1	ks	Instalace.
.
 	10 890,00	
1	ks	Balné a dopravné, dodací podmínka DDP
Praha 6 - Suchdol dle Incoterms 2010.
.
 	3 630,00	

Celková cena s DPH: 796 785,00 Kč

Bedřich PRAJZLER 
Vedoucí zásobování

Ústav chemických procesů AV ČR, v.v.i.
Rozvojová 135, 165 02 Praha 6
IČ : 67985858  DIČ : CZ67985858
e-mail:       prajzler@icpf.cas.cz
telefon:     220 390 228
mobil:        773 400 194

						Razítko a podpis: