Serverové chassis lks

***s****is*

|  |  |  |
| --- | --- | --- |
| ***Partnumber (PN}*** | ***Komponent*** | ***Počet komponent v* lks *Serverového chas*** |
| 8721HC2 | Chassis : Lenovo Flex System Enterprise Chassis w/CMM2 | 1 |
| ASUS | Lenovo Flex System Enterprise Chassis w/ CMM2 | 1 |
| ASUX | System Documentation and Software-US English | 1 |
| A3DP | Lenovo Flex System FC5022 24-port 16Gb.SAN Scalable Sw | 2 |
| ASUU | Lenovo Flex System Fabric EN4093R 10Gb Scalable Switch | 2 |
| ASQ8 | Lenovo Flex System Redundant Chassis Management Med | 1 |
| 5053 | SFP+ SR Transceiver | **4** |
| A22R | Brocade 16Gb SFP+ Optical Transceiver | 16 |
| AlNF | System Console Breakout Cable | 1 |
| AOUC | Flex System Enterprise Chassis 2500W Power Module Stan | 2 |
| AOUD | Flex System Enterprise Chassis 2500W Power Module | 4 |
| AOUA | Flex System Enterprise Chassis 80mm Fan Module | **4** |
| AOTP | Flex System Compute Node Filler | 13 |
| ASPT | Lenovo Flex System Chassis Management Module 2 | 1 |
| ASUW | Lenovo Flex System Enterprise Chassis Label Group | 1 |
| AlOX | Flex System Enterprise Chassis Rack Kit | 1 |
| ASVB | Lenovo Flex System Enterprise Chassis Packaging World W | 1 |
| OOX8553 | Essential Service - 3Yr 24x7 4Hr Response | 1 |
|  |  |  |
| Servery typu Blade 4ks |  |  |
| ***Partnumber (PN}*** | ***IKomaonent*** | ***komponent v* lks *serveru typu Slad*** |
| 7X16CT01WW | Node: ThinkSystem SN550 - 3yr Warranty | 1 |
| AUXP | Lenovo ThinkSystem SN550 Server | 1 |
| AX7D | Intel Xeon Gold 5118 12C 105W 2.3GHz Processor | 2 |
| AUND | ThinkSystem 32GB TruDDR4 2666 MHz (2Rx4 1.2V) RDIMtv | 8 |
| AUYR | ThinkSystem RAID 530-4i 2 Drive Adapter Kit for SN550 | 1 |
| 5977 | Select Storage devices - no configured RAID required | 1 |
| B498 | ThinkSystem 2.5" Intel S4510 240GB Entry SATA 6Gb Hot S | 2 |
| AUMV | ThinkSystem M.2 with Mirroring Enablement Kit | 1 |
| AUUL | ThinkSystem M.2 CVl 32GB SATA 6Gbps Non-Hot Swap SSI | 2 |
| AUYN | ThinkSystem SN550/SN850 Fabric Connector | 1 |
| AVCW | ThinkSystem Emulex LPm16002B-L Mezz 16Gb 2-Port Fibre | 1 |
| BOMJ | Feature Enable TPM 1.2 | 1 |
| AV2Q | Lenovo ThinkSystem SN550 Server WW packaging - Standa | 1 |
| AULQ | ThinkSystem lU CPU Performance Heatsink | 1 |
| AUYl | Lenovo ThinkSystem SN550 Server Label | 1 |
| AVUN | Lenovo ThinkSystem SN550 Server Service LabeI LI | 1 |
| AVJ2 | ThinkSystem 4R CPU HS Clip | 2 |
| AUXY | Lenovo ThinkSystem Server HDD Bezel Facia | 1 |
| AUYO | Lenovo ThinkSystem SN550 Server Cover | 1 |
| AUY3 | Lenovo ThinkSystem SN550 Server Air Baffle | 1 |
| AV2U | Lenovo ThinkSystem Server Rear CPU Heatsink | 1 |
| AXHD | Intel lnside Xeon Label | 1 |
| BOML | Feature Enable TPM on MB | 1 |
| AV2S | System Documentation | 1 |
| 5WS7A01892 | Foundation Service - 3Yr Next Business Day Response | 1 |

***e***