**Příloha č. 1**

**ke smlouvě o dílo č. 11/2019**

1. **Technická specifikace předmětu veřejné zakázky**

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  | **počet** |
| **1.1** | **Core switche(C13\_Europe)\_Site1** | |  |
|  | **S6700 Series Ethernet Switches** | | **2** |
|  | **Mainframe** | |  |
|  | S6720-32C-SI-AC | S6720-32C-SI Bundle(24 Ethernet 100M/1/2.5/5/10G ports,4 10 Gig SFP+,with 1 interface slot,with 150W AC power supply) |  |
|  | **Power** | |  |
|  | ES0W2PSA0150 | 150W AC Power Module(Black) |  |
|  | **Interface Card** | |  |
|  | ES5D21Q02Q00 | 2-port 40GE QSFP+ interface card (used in S6720SI, S6320SI, S5330HI, and S5730HI series) |  |
|  | **High Speed Cable** | |  |
|  | **QSFP+ High Speed Cable** | |  |
|  | QSFP-40G-CU1M | QSFP+,40G,High Speed Direct-attach Cables,1m,QSFP+38M,CC8P0.254B(S),QSFP+38M,Used indoor |  |
|  | **Technical Support Service** | |  |
|  | 98010715-88134UJL-12 | S6720-32C-SI Bundle(24 Ethernet 100M/1/2.5/5/10G ports,4 10 Gig SFP+,with 1 interface slot,with 150W AC power supply)-Hi-Care Standard 9x5xNBD Service-12Month(s) |  |
|  |  |  |  |
| **1.2** | **Switch Serverovna(C13\_Europe)\_Site1** | |  |
|  | **S5700 Series Ethernet Switches** | | **3** |
|  | **Mainframe** | |  |
|  | **S57 LI Series Mainframe** | |  |
|  | S5720-52X-LI-AC | S5720-52X-LI-AC(48 Ethernet 10/100/1000 ports,4 10 Gig SFP+,AC power support) |  |
|  | **High Speed Cable** | |  |
|  | **SFP+ High Speed Cable** | |  |
|  | SFP-10G-CU1M | SFP+,10G,High Speed Direct-attach Cables,1m,SFP+20M,CC2P0.254B(S),SFP+20M,Used indoor |  |
|  | **Technical Support Service** | |  |
|  | 98010606-88134UJL-12 | S5720-52X-LI-AC(48 Ethernet 10/100/1000 ports,4 10 Gig SFP+,AC power support)-Hi-Care Standard 9x5xNBD Service-12Month(s) |  |
|  |  |  |  |
| **1.3** | **Switch Serverovna PoE(C13\_Europe)\_Site1** | |  |
|  | **S5700 Series Ethernet Switches** | | **1** |
|  | **Mainframe** | |  |
|  | **S57 LI Series Mainframe** | |  |
|  | S5720-52X-PWR-LI-AC | S5720-52X-PWR-LI-AC(48 Ethernet 10/100/1000 ports,4 10 Gig SFP+,PoE+,370W POE AC power support) |  |
|  | **High Speed Cable** | |  |
|  | **SFP+ High Speed Cable** | |  |
|  | SFP-10G-CU1M | SFP+,10G,High Speed Direct-attach Cables,1m,SFP+20M,CC2P0.254B(S),SFP+20M,Used indoor |  |
|  | **Technical Support Service** | |  |
|  | 98010619-88134UJL-12 | S5720-52X-PWR-LI-AC(48 Ethernet 10/100/1000 ports,4 10 Gig SFP+,PoE+,370W POE AC power support)-Hi-Care Standard 9x5xNBD Service-12Month(s) |  |
|  |  |  |  |
| **1.4** | **Switch 1. patro(C13\_Europe)\_Site1** | |  |
|  | **S5700 Series Ethernet Switches** | | **1** |
|  | **Mainframe** | |  |
|  | **S57 LI Series Mainframe** | |  |
|  | S5720-28X-PWR-LI-AC | S5720-28X-PWR-LI-AC(24 Ethernet 10/100/1000 ports,4 10 Gig SFP+,PoE+,370W POE AC power support) |  |
|  | **Technical Support Service** | |  |
|  | 98010593-88134UJL-12 | S5720-28X-PWR-LI-AC(24 Ethernet 10/100/1000 ports,4 10 Gig SFP+,PoE+,370W POE AC power support)-Hi-Care Standard 9x5xNBD Service-12Month(s) |  |
|  |  |  |  |
| **1.5** | **Switch 2. a 3. patro PoE(C13\_Europe)\_Site1** | |  |
|  | **S5700 Series Ethernet Switches** | | **2** |
|  | **Mainframe** | |  |
|  | **S57 LI Series Mainframe** | |  |
|  | S5720-52X-PWR-LI-AC | S5720-52X-PWR-LI-AC(48 Ethernet 10/100/1000 ports,4 10 Gig SFP+,PoE+,370W POE AC power support) |  |
|  | **Technical Support Service** | |  |
|  | 98010619-88134UJL-12 | S5720-52X-PWR-LI-AC(48 Ethernet 10/100/1000 ports,4 10 Gig SFP+,PoE+,370W POE AC power support)-Hi-Care Standard 9x5xNBD Service-12Month(s) |  |
|  |  |  |  |
| **1.6** | **Switch Přístavba PoE(C13\_Europe)\_Site1** | |  |
|  | **S5700 Series Ethernet Switches** | | **1** |
|  | **Mainframe** | |  |
|  | **S57 LI Series Mainframe** | |  |
|  | S5720-52X-PWR-LI-AC | S5720-52X-PWR-LI-AC(48 Ethernet 10/100/1000 ports,4 10 Gig SFP+,PoE+,370W POE AC power support) |  |
|  | **Technical Support Service** | |  |
|  | 98010619-88134UJL-12 | S5720-52X-PWR-LI-AC(48 Ethernet 10/100/1000 ports,4 10 Gig SFP+,PoE+,370W POE AC power support)-Hi-Care Standard 9x5xNBD Service-12Month(s) |  |
|  |  |  |  |
| **1.7** | **Switch Brno(C13\_Europe)\_Site1** | |  |
|  | **S5700 Series Ethernet Switches** | | **1** |
|  | **Mainframe** | |  |
|  | **S57 LI Series Mainframe** | |  |
|  | S5720-52X-LI-AC | S5720-52X-LI-AC(48 Ethernet 10/100/1000 ports,4 10 Gig SFP+,AC power support) |  |
|  | **Technical Support Service** | |  |
|  | 98010606-88134UJL-12 | S5720-52X-LI-AC(48 Ethernet 10/100/1000 ports,4 10 Gig SFP+,AC power support)-Hi-Care Standard 9x5xNBD Service-12Month(s) |  |
|  |  |  |  |
| **1.8** | **Switch Pardubice(C13\_Europe)\_Site1** | |  |
|  | **S5700 Series Ethernet Switches** | | **1** |
|  | **Mainframe** | |  |
|  | **S57 LI Series Mainframe** | |  |
|  | S5720-28X-LI-AC | S5720-28X-LI-AC(24 Ethernet 10/100/1000 ports,4 10 Gig SFP+,AC power support) |  |
|  | **Technical Support Service** | |  |
|  | 98010581-88134UJL-12 | S5720-28X-LI-AC(24 Ethernet 10/100/1000 ports,4 10 Gig SFP+,AC power support)-Hi-Care Standard 9x5xNBD Service-12Month(s) |  |
|  |  |  |  |
| **1.9** | **S5700 Spares\_Site1** | |  |
|  | **S5700 Series Ethernet Switches** | | **1** |
|  | **Optical Transceiver** | |  |
|  | **GE-SFP Optical Transceiver** | |  |

1. **Doba a místo plnění veřejné zakázky**

Předpokládaná doba plnění veřejné zakázky: dodávka nejpozději do 18.4.2019

Místa plnění veřejné zakázky: Žabovřeská 250, 156 00 Praha 5 – Zbraslav

Lidická 25/27, 602 00 Brno-střed

B. Němcové 231, 530 02 Pardubice V-Zelené Předměstí

1. **Specifikace záruk**

Záruky dodávaného hardware a software jsou poskytovány výrobcem, popisy jsou uvedeny na jeho webových stránkách. Hlášení závad probíhá pomocí kontaktů uvedených na stránkách výrobce. Typy a úrovně záruk jsou uvedeny u jednotlivých specifikovaných položek v bodě 1 této přílohy.

|  |  |
| --- | --- |
| Za Zhotovitele:  V Praze dne: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_2019  Ing. Zbyněk Juřena, Předseda představenstva | Za Objednatele:  V Praze dne: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_2019  doc. Ing. Radim Vácha, Ph.D., ředitel |