|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **ISO-KF** | **DN** |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  | **Výrobce** | **Obchodní název** |  | **Objednávací číslo** |  | **Minimální počet [ks]** | **Odhadovaný počet [ks]** |  | **Cena za kus bez DPH** |  | **Celková cena bez DPH** |
| **Komponenty ISO-KF dle ISO 2861/1** | |  |  |  |  | [€] |  | [€] |
| **Clamping ring - wing nut** | 10-16 |  | Hositrad | KF Clamps |  | KF16/C |  | 0 | 5 |  |  |  | 0,00 |
| **Materiál:** | 20-25 |  | Hositrad | KF Clamps |  | KF25/C |  | 5 | 10 |  |  |  | 0,00 |
| Clamping ring half: aluminum 380.0 or Aluminum ADC 12 | 32-40 |  | Hositrad | KF Clamps |  | KF40/C |  | 10 | 30 |  |  |  | 0,00 |
| Bolt: steel nickel plate, Nut: zinc alloy nickel plated | 50 |  | Hositrad | KF Clamps |  | KF50/C |  | 0 | 5 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Centering ring** | 10 |  | Hositrad | KF Centering Ring with Viton O-Ring - SST 304 |  | KF10/R |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 16 |  | Hositrad | KF Centering Ring with Viton O-Ring - SST 304 |  | KF16/R |  | 0 | 1 |  |  |  | 0,00 |
| Ring: AISI 304 or AISI 316L; Seal: elastomer FPM | 25 |  | Hositrad | KF Centering Ring with Viton O-Ring - SST 304 |  | KF25/R |  | 0 | 1 |  |  |  | 0,00 |
|  | 40 |  | Hositrad | KF Centering Ring with Viton O-Ring - SST 304 |  | KF40/R |  | 0 | 1 |  |  |  | 0,00 |
|  | 50 |  | Hositrad | KF Centering Ring with Viton O-Ring - SST 304 |  | KF50/R |  | 0 | 5 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Centering ring** | 10 |  | Hositrad | KF Centering Ring with Viton O-Ring - Alu |  | KF10/RA |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 16 |  | Hositrad | KF Centering Ring with Viton O-Ring - Alu |  | KF16/RA |  | 0 | 1 |  |  |  | 0,00 |
| Ring: Aluminum 6061 or 6026 ; Seal: elastomer FPM | 25 |  | Hositrad | KF Centering Ring with Viton O-Ring - Alu |  | KF25/RA |  | 10 | 15 |  |  |  | 0,00 |
|  | 40 |  | Hositrad | KF Centering Ring with Viton O-Ring - Alu |  | KF40/RA |  | 20 | 30 |  |  |  | 0,00 |
|  | 50 |  | Hositrad | KF Centering Ring with Viton O-Ring - Alu |  | KF50/RA |  | 0 | 5 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Blank flange** | 10 |  | Hositrad | Blank Flange Stailess Steel 304 |  | KF10/B |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 16 |  | Hositrad | Blank Flange Stailess Steel 304 |  | KF16/B |  | 0 | 1 |  |  |  | 0,00 |
| AISI 304 or AISI 316L | 25 |  | Hositrad | Blank Flange Stailess Steel 304 |  | KF25/B |  | 0 | 10 |  |  |  | 0,00 |
|  | 40 |  | Hositrad | Blank Flange Stailess Steel 304 |  | KF40/B |  | 0 | 10 |  |  |  | 0,00 |
|  | 50 |  | Hositrad | Blank Flange Stailess Steel 304 |  | KF50/B |  | 0 | 5 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Blank flange** | 10 |  | Hositrad | Blank Flange Aluminium |  | KF10/BA |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 16 |  | Hositrad | Blank Flange Aluminium |  | KF16/BA |  | 0 | 3 |  |  |  | 0,00 |
| Aluminum 6082 or Aluminum 6061 T6 | 25 |  | Hositrad | Blank Flange Aluminium |  | KF25/BA |  | 0 | 5 |  |  |  | 0,00 |
|  | 40 |  | Hositrad | Blank Flange Aluminium |  | KF40/BA |  | 0 | 5 |  |  |  | 0,00 |
|  | 50 |  | Hositrad | Blank Flange Aluminium |  | KF50/BA |  | 0 | 3 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Elbow 90°** | 10 |  | Hositrad | Elbow KF 90° |  | KE10/13 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 16 |  | Hositrad | Elbow KF 90° |  | KE16/20 |  | 0 | 1 |  |  |  | 0,00 |
| AISI 304 | 25 |  | Hositrad | Elbow KF 90° |  | KE25/28 |  | 0 | 5 |  |  |  | 0,00 |
|  | 40 |  | Hositrad | Elbow KF 90° |  | KE40/44 |  | 0 | 5 |  |  |  | 0,00 |
|  | 50 |  | Hositrad | Elbow KF 90° |  | KE50/54 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Elbow 90°** | 16 |  | Hositrad | Elbow KF 90° Aluminium |  | KE16/19 Alu |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 25 |  | Hositrad | Elbow KF 90° Aluminium |  | KE25/25 Alu |  | 2 | 5 |  |  |  | 0,00 |
| Aluminum 6082 or Aluminum 6061 T6 | 40 |  | Hositrad | Elbow KF 90° Aluminium |  | KE40/38 Alu |  | 2 | 5 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Elbow 45°** | 16 |  | Hositrad | Elbow KF 45° |  | KE16/20-45 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 25 |  | Hositrad | Elbow KF 45° |  | KE25/25-45 |  | 2 | 5 |  |  |  | 0,00 |
| AISI 304 | 40 |  | Hositrad | Elbow KF 45° |  | KE40/44-45 |  | 2 | 5 |  |  |  | 0,00 |
|  | 50 |  | Hositrad | Elbow KF 45° |  | KE50/54-45 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Tee** | 10 |  | Hositrad | Tee Equal |  | KT10/13 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 16 |  | Hositrad | Tee Equal |  | KT16/20 |  | 0 | 1 |  |  |  | 0,00 |
| AISI 304 | 25 |  | Hositrad | Tee Equal |  | KT25/28 |  | 0 | 5 |  |  |  | 0,00 |
|  | 40 |  | Hositrad | Tee Equal |  | KT40/44 |  | 0 | 5 |  |  |  | 0,00 |
|  | 50 |  | Hositrad | Tee Equal |  | KT50/54 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Tee** | 10 |  | Hositrad | Tee Equal |  | KT10/13 Alu |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 16 |  | Hositrad | Tee Equal |  | KT16/19 Alu |  | 2 | 5 |  |  |  | 0,00 |
| Aluminum 6082 or Aluminum 6061 T6 | 25 |  | Hositrad | Tee Equal |  | KT25/25 Alu |  | 2 | 5 |  |  |  | 0,00 |
|  | 40 |  | Hositrad | Tee Equal |  | KT40/38 Alu |  | 2 | 5 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Reducing Tee** | 25/16 |  | Hositrad | Tee Reducer |  | KTR25/16 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 40/16 |  | Hositrad | Tee Reducer |  | KTR40/16 |  | 0 | 1 |  |  |  | 0,00 |
| AISI 304 | 40/25 |  | Hositrad | Tee Reducer |  | KTR40/25 |  | 1 | 1 |  |  |  | 0,00 |
|  | 50/16 |  | Hositrad | Tee Reducer |  | KTR50/16 |  | 0 | 1 |  |  |  | 0,00 |
|  | 50/25 |  | Hositrad | Tee Reducer |  | KTR50/25 |  | 0 | 1 |  |  |  | 0,00 |
|  | 50/40 |  | Hositrad | Tee Reducer |  | KTR50/40 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Cross** | 16 |  | Hositrad | Cross Equal 4-way |  | KX4/16/20 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 25 |  | Hositrad | Cross Equal 4-way |  | KX4/25/28 |  | 0 | 1 |  |  |  | 0,00 |
| AISI 304 | 40 |  | Hositrad | Cross Equal 4-way |  | KX4/40/44 |  | 0 | 2 |  |  |  | 0,00 |
|  | 50 |  | Hositrad | Cross Equal 4-way |  | KX4/50/57 |  | 0 | 2 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Cross** | 16 |  | Hositrad | Cross Equal 4-way |  | KX4/16/19 Alu |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 25 |  | Hositrad | Cross Equal 4-way |  | KX4/25/25 Alu |  | 0 | 5 |  |  |  | 0,00 |
| Aluminum 6082 or Aluminum 6061 T6 | 40 |  | Hositrad | Cross Equal 4-way |  | KX4/40/38 Alu |  | 0 | 5 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Straight Reducer** | 25/16 |  | Hositrad | Reducers |  | KFA16/25 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 40/16 |  | Hositrad | Reducers |  | KFA16/40 |  | 0 | 1 |  |  |  | 0,00 |
| AISI 304 or AISI 303 | 40/25 |  | Hositrad | Reducers |  | KFA25/40 |  | 0 | 3 |  |  |  | 0,00 |
|  | 50/16 |  | Hositrad | Reducers |  | KFA16/50 |  | 0 | 1 |  |  |  | 0,00 |
|  | 50/25 |  | Hositrad | Reducers |  | KFA25/50 |  | 0 | 1 |  |  |  | 0,00 |
|  | 50/40 |  | Hositrad | Reducers |  | KFA40/50 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Straight Reducer** | 25/16 |  | Hositrad | Reducers |  | KFA16/25A |  | 2 | 5 |  |  |  | 0,00 |
| **Materiál:** | 40/16 |  | Hositrad | Reducers |  | KFA16/40A |  | 0 | 1 |  |  |  | 0,00 |
| Aluminum 6082 or Aluminum 6061 T6 | 40/25 |  | Hositrad | Reducers |  | KFA25/40A |  | 3 | 5 |  |  |  | 0,00 |
|  | 50/25 |  | Hositrad | Reducers |  | KFA25/50A |  | 0 | 1 |  |  |  | 0,00 |
|  | 50/40 |  | Hositrad | Reducers |  | KFA40/50A |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Metal hose** | 16/250 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX16/250 |  | 0 | 1 |  |  |  | 0,00 |
| NOTE: | 16/500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX16/500 |  | 0 | 1 |  |  |  | 0,00 |
| - DN/length | 16/750 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX16/750 |  | 0 | 1 |  |  |  | 0,00 |
| - hose is not shrinking under vacuum(hadice které se pod vakuem nesmršťují) | 16/1000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX16/1000 |  | 0 | 1 |  |  |  | 0,00 |
|  | 16/1500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX16/1500 |  | 0 | 1 |  |  |  | 0,00 |
|  | 16/2000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX16/2000 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 25/250 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX25/250 |  | 0 | 1 |  |  |  | 0,00 |
| Flange: AISI 304 or AISI 316L | 25/500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX25/500 |  | 0 | 1 |  |  |  | 0,00 |
| Bellows: AISI 304 or AISI 316L | 25/750 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX25/750 |  | 0 | 1 |  |  |  | 0,00 |
|  | 25/1000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX25/1000 |  | 0 | 1 |  |  |  | 0,00 |
|  | 25/1500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX25/1500 |  | 0 | 1 |  |  |  | 0,00 |
|  | 25/2000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX25/2000 |  | 0 | 1 |  |  |  | 0,00 |
|  | 40/250 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX40/250 |  | 0 | 1 |  |  |  | 0,00 |
|  | 40/500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX40/500 |  | 0 | 1 |  |  |  | 0,00 |
|  | 40/750 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX40/750 |  | 0 | 1 |  |  |  | 0,00 |
|  | 40/1000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX40/1000 |  | 0 | 1 |  |  |  | 0,00 |
|  | 40/1500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX40/1500 |  | 0 | 1 |  |  |  | 0,00 |
|  | 40/2000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX40/2000 |  | 0 | 1 |  |  |  | 0,00 |
|  | 50/250 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX50/250 |  | 0 | 1 |  |  |  | 0,00 |
|  | 50/500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX50/500 |  | 0 | 1 |  |  |  | 0,00 |
|  | 50/750 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX50/750 |  | 0 | 1 |  |  |  | 0,00 |
|  | 50/1000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX50/1000 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Metal hose, Flexible** | 16/250 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX16/250 |  | 0 | 1 |  |  |  | 0,00 |
| NOTE: | 16/500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX16/500 |  | 0 | 1 |  |  |  | 0,00 |
| - DN/length | 16/750 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX16/750 |  | 0 | 1 |  |  |  | 0,00 |
| - hose is shrinking under vacuum(hadice které se pod vakuem smršťují) | 16/1000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX16/1000 |  | 0 | 1 |  |  |  | 0,00 |
|  | 25/250 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX25/250 |  | 0 | 1 |  |  |  | 0,00 |
|  | 25/500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX25/500 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 25/750 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX25/750 |  | 0 | 1 |  |  |  | 0,00 |
| Flange: AISI 304 or AISI 316L | 25/1000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX25/1000 |  | 0 | 1 |  |  |  | 0,00 |
| Bellows: AISI 304 or AISI 316L | 40/250 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX40/250 |  | 0 | 1 |  |  |  | 0,00 |
|  | 40/500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX40/500 |  | 0 | 1 |  |  |  | 0,00 |
|  | 40/750 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX40/750 |  | 0 | 1 |  |  |  | 0,00 |
|  | 40/1000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX40/1000 |  | 0 | 1 |  |  |  | 0,00 |
|  | 50/250 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX50/250 |  | 0 | 1 |  |  |  | 0,00 |
|  | 50/500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | KX50/500 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Adaptor ISO-KF/ISO-K** | 25/63 |  | Hositrad | Adaptor to KF |  | ISO63/25A |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 40/63 |  | Hositrad | Adaptor to KF |  | ISO63/40A |  | 1 | 2 |  |  |  | 0,00 |
| AISI 304 | 50/63 |  | Hositrad | Adaptor to KF |  | ISO63/50A |  | 1 | 2 |  |  |  | 0,00 |
|  | 40/100 |  | Hositrad | Adaptor to KF |  | ISO100/40A |  | 2 | 3 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Claw Clamp KF** | 10-50 |  | Hositrad | KF Clamps Nail |  | KF10/KF50/NC |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Aluminum 6081 or Aluminum 6061 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Adaptor ISO-CF/KF** | 16/16 |  | Hositrad | Adaptors CF to KF |  | CFA16/KF16 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 16/25 |  | Hositrad | Adaptors CF to KF |  | CFA16/KF25 |  | 0 | 1 |  |  |  | 0,00 |
| AISI 304 | 40/16 |  | Hositrad | Adaptors CF to KF |  | CFA35/KF16 |  | 0 | 1 |  |  |  | 0,00 |
|  | 40/25 |  | Hositrad | Adaptors CF to KF |  | CFA35/KF25 |  | 0 | 1 |  |  |  | 0,00 |
|  | 40/40 |  | Hositrad | Adaptors CF to KF |  | CFA35/KF40 |  | 0 | 1 |  |  |  | 0,00 |
|  | 63/40 |  | Hositrad | Adaptors CF to KF |  | CFA63/KF40 |  | 0 | 1 |  |  |  | 0,00 |
|  | 100/40 |  | Hositrad | Adaptors CF to KF |  | CFA100/KF40 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  | **Celková cena** |  | **5 831,90 €** |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  | **Celková cena bez DPH** | | |
|  |  |  |  |  |  |  |  |  |  |  | **Standardní komponenty** | | **34 472,30 €** |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **ISO-K** | **DN** |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  | **Výrobce** | **Obchodní název** |  | **Objednávací číslo** |  | **Minimální počet [ks]** | **Odhadovaný počet [ks]** |  | **Cena za kus bez DPH** |  | **Celková cena bez DPH** |
| **Komponenty ISO-K a ISO-F dle ISO 1609** | |  |  |  |  | [€] |  | [€] |
| **Double clamp** | 63-250 |  | Hositrad | Clamp Double Claw ISO-K, Steinless Steel |  | ISO63C/SS |  | 0 | 10 |  |  |  | 0,00 |
| **Materiál:** | 320-500 |  | Hositrad | Clamp Double Claw ISO-K, Steinless Steel |  | ISO320C/SS |  | 0 | 10 |  |  |  | 0,00 |
| AISI 316 | 630 |  | Hositrad | Clamp Double Claw ISO-K, Steinless Steel |  | ISO630C/SS |  | 0 | 10 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Double clamp** | 63-250 |  | Hositrad | Clamp Double Claw ISO-K, Zinc Plated |  | ISO63C |  | 200 | 500 |  |  |  | 0,00 |
| **Materiál:** | 320-500 |  | Hositrad | Clamp Double Claw ISO-K, Zinc Plated |  | ISO320C |  | 50 | 200 |  |  |  | 0,00 |
| Zinc-plate Steel 1045 | 630 |  | Hositrad | Clamp Double Claw ISO-K, Zinc Plated |  | ISO630C |  | 0 | 10 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Single clamp - For a base plate with O-ring** | 160-250 |  | Hositrad | Clamp Single Wall ISO-K, Aluminium |  | ISO160/CA |  | 0 | 10 |  |  |  | 0,00 |
| **Clamp Materiál:** |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Aluminum 6082, Aluminum 6061 or Aluminum 6061 T6 |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Single clamp - For a base plate with O-ring** | 63-100 |  | Hositrad | Clamp Single Wall ISO-K, Zinc Plated Steel |  | ISO63/CG |  | 0 | 50 |  |  |  | 0,00 |
| **Clamp Materiál:** | 160-250 |  | Hositrad | Clamp Single Wall ISO-K, Zinc Plated Steel |  | ISO160/CG |  | 0 | 50 |  |  |  | 0,00 |
| Zinc-plate Steel 1045 | 320-500 |  | Hositrad | Clamp Single Wall ISO-K, Zinc Plated Steel |  | ISO320/CG |  | 0 | 10 |  |  |  | 0,00 |
|  | 630 |  | Hositrad | Clamp Single Wall ISO-K, Zinc Plated Steel |  | ISO630/CG |  | 0 | 10 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Single clamp - Base plate with sealing groove** | 63-100 |  | Hositrad | Clamp Single Wall ISO-K, Zinc Plated Steel |  | ISO63/CGS |  | 0 | 10 |  |  |  | 0,00 |
| **Clamp Materiál:** | 160-250 |  | Hositrad | Clamp Single Wall ISO-K, Zinc Plated Steel |  | ISO160/CGS |  | 0 | 10 |  |  |  | 0,00 |
| Zinc-plate Steel 1045 | 320-500 |  | Hositrad | Clamp Single Wall ISO-K, Zinc Plated Steel |  | ISO320/CGS |  | 0 | 10 |  |  |  | 0,00 |
|  | 630 |  | Hositrad | Clamp Single Wall ISO-K, Zinc Plated Steel |  | ISO630/CGS |  | 0 | 10 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Centering ring with outer ring** | 63 |  | Hositrad | Ring Centering ISO-K |  | ISO63SV |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 80 |  | Hositrad | Ring Centering ISO-K |  | ISO80SV |  | 0 | 1 |  |  |  | 0,00 |
| Inner ring: AISI 304 or AISI 316Ti | 100 |  | Hositrad | Ring Centering ISO-K |  | ISO100SV |  | 0 | 1 |  |  |  | 0,00 |
| Outer ring: Aluminum 6082 or Aluminum 6061 T6 | 160 |  | Hositrad | Ring Centering ISO-K |  | ISO160SV |  | 0 | 1 |  |  |  | 0,00 |
| Seal: elastomer FPM | 200 |  | Hositrad | Ring Centering ISO-K |  | ISO200SV |  | 0 | 1 |  |  |  | 0,00 |
|  | 250 |  | Hositrad | Ring Centering ISO-K |  | ISO250SV |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Centering ring with outer ring** | 63 |  | Hositrad | Ring Centering ISO-K |  | ISO63AV |  | 0 | 5 |  |  |  | 0,00 |
| **Materiál:** | 80 |  | Hositrad | Ring Centering ISO-K |  | ISO80AV |  | 0 | 15 |  |  |  | 0,00 |
| Inner ring: Aluminum 6082 or Aluminum 6061 T6 | 100 |  | Hositrad | Ring Centering ISO-K |  | ISO100AV |  | 20 | 80 |  |  |  | 0,00 |
| Outer ring: Aluminum 6082 or Aluminum 6061 T6 | 160 |  | Hositrad | Ring Centering ISO-K |  | ISO160AV |  | 20 | 80 |  |  |  | 0,00 |
| Seal: elastomer FPM | 200 |  | Hositrad | Ring Centering ISO-K |  | ISO200AV |  | 0 | 1 |  |  |  | 0,00 |
|  | 250 |  | Hositrad | Ring Centering ISO-K |  | ISO250AV |  | 0 | 10 |  |  |  | 0,00 |
|  | 320 |  | Hositrad | Ring Centering ISO-K |  | ISO320AV |  | 0 | 3 |  |  |  | 0,00 |
|  | 400 |  | Hositrad | Ring Centering ISO-K |  | ISO400AV |  | 0 | 1 |  |  |  | 0,00 |
|  | 500 |  | Hositrad | Ring Centering ISO-K |  | ISO500AV |  | 0 | 1 |  |  |  | 0,00 |
|  | 630 |  | Hositrad | Ring Centering ISO-K |  | ISO630AV |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Blank flange** | 63 |  | Hositrad | Flange Blank ISO-K |  | ISO63B |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 80 |  | Hositrad | Flange Blank ISO-K |  | ISO80B |  | 0 | 1 |  |  |  | 0,00 |
| AISI 304 | 100 |  | Hositrad | Flange Blank ISO-K |  | ISO100B |  | 0 | 5 |  |  |  | 0,00 |
|  | 160 |  | Hositrad | Flange Blank ISO-K |  | ISO160B |  | 0 | 1 |  |  |  | 0,00 |
|  | 200 |  | Hositrad | Flange Blank ISO-K |  | ISO200B |  | 0 | 1 |  |  |  | 0,00 |
|  | 250 |  | Hositrad | Flange Blank ISO-K |  | ISO250B |  | 0 | 1 |  |  |  | 0,00 |
|  | 320 |  | Hositrad | Flange Blank ISO-K |  | ISO320B |  | 0 | 1 |  |  |  | 0,00 |
|  | 400 |  | Hositrad | Flange Blank ISO-K |  | ISO400B |  | 0 | 1 |  |  |  | 0,00 |
|  | 500 |  | Hositrad | Flange Blank ISO-K |  | ISO500B |  | 0 | 1 |  |  |  | 0,00 |
|  | 630 |  | Hositrad | Flange Blank ISO-K |  | ISO630B |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Blank flange** | 63 |  | Hositrad | Flange Blank ISO-K |  | ISO63BA |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 80 |  | Hositrad | Flange Blank ISO-K |  | ISO80BA |  | 0 | 1 |  |  |  | 0,00 |
| Aluminum 6082 or Aluminum 6061 T6 | 100 |  | Hositrad | Flange Blank ISO-K |  | ISI100BA |  | 0 | 1 |  |  |  | 0,00 |
|  | 160 |  | Hositrad | Flange Blank ISO-K |  | ISO160BA |  | 0 | 1 |  |  |  | 0,00 |
|  | 200 |  | Hositrad | Flange Blank ISO-K |  | ISO200BA |  | 0 | 1 |  |  |  | 0,00 |
|  | 250 |  | Hositrad | Flange Blank ISO-K |  | ISO250BA |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Elbow 90°** | 63 (88) |  | Hositrad | ISO-K Elbow 90° |  | ISO63/E |  | 0 | 1 |  |  |  | 0,00 |
| **Note: DN (Center to End Dimension)** | 100 (108) |  | Hositrad | ISO-K Elbow 90° |  | ISO100/E |  | 0 | 5 |  |  |  | 0,00 |
| **Materiál:** AISI 304 | 160 (138) |  | Hositrad | ISO-K Elbow 90° |  | ISO160/EM |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Tee** | 63 (176) |  | Hositrad | Tee Equal ISO-K |  | ISO63/T |  | 0 | 1 |  |  |  | 0,00 |
| **Note: DN (Length)** | 100 (216) |  | Hositrad | Tee Equal ISO-K |  | ISO100/T |  | 0 | 5 |  |  |  | 0,00 |
| **Materiál:** AISI 304 | 160 (276) |  | Hositrad | Tee Equal ISO-K |  | ISO160/T |  | 0 | 2 |  |  |  | 0,00 |
|  | 200 (356) |  | Hositrad | Tee Equal ISO-K |  | ISO200/T |  | 0 | 1 |  |  |  | 0,00 |
|  | 250 (416) |  | Hositrad | Tee Equal ISO-K |  | ISO250/T |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Reducing Tee** | 100/63 (216) |  | Hositrad | Tee Reducer ISO |  | ISO100/63TR |  | 0 | 3 |  |  |  | 0,00 |
| **Note: DN/DN (Length)** | 160/63 (276) |  | Hositrad | Tee Reducer ISO |  | ISO160/63TR |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** AISI 304 | 160/100 (276) |  | Hositrad | Tee Reducer ISO |  | ISO160/100TR |  | 0 | 3 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Cross** | 63 (176) |  | Hositrad | Cross Equal 4-way ISO-K |  | ISOX4/63 |  | 0 | 1 |  |  |  | 0,00 |
| **Note: DN (Length)** | 100 (216) |  | Hositrad | Cross Equal 4-way ISO-K |  | ISOX4/100 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** AISI 304 | 160 (276) |  | Hositrad | Cross Equal 4-way ISO-K |  | ISOX4/160 |  | 0 | 1 |  |  |  | 0,00 |
|  | 200 (356) |  | Hositrad | Cross Equal 4-way ISO-K |  | ISOX4/200 |  | 0 | 1 |  |  |  | 0,00 |
|  | 250 (416) |  | Hositrad | Cross Equal 4-way ISO-K |  | ISOX4/250 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Reducer, Straight** | 80/63 |  | Hositrad | Reducer |  | ISO63/80R |  | 0 | 1 |  |  |  | 0,00 |
| **Note: DN/DN (Length)** | 100/63 (50) |  | Hositrad | Reducer |  | ISO63/100R |  | 1 | 3 |  |  |  | 0,00 |
| **Materiál:** AISI 303 or AISI 304 | 160/100 (50) |  | Hositrad | Reducer |  | ISO100/160R |  | 1 | 3 |  |  |  | 0,00 |
|  | 200/160 (50) |  | Hositrad | Reducer |  | ISO160/200R |  | 0 | 1 |  |  |  | 0,00 |
|  | 250/160 (50) |  | Hositrad | Reducer |  | ISO160/250R |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Metal hose** | 63/250 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | ISOX63/250 |  | 0 | 1 |  |  |  | 0,00 |
| NOTE: | 63/500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | ISOX63/500 |  | 0 | 1 |  |  |  | 0,00 |
| - DN/length | 63/750 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | ISOX63/750 |  | 0 | 1 |  |  |  | 0,00 |
| - Hose is not shrinking under vacuum(hadice které se pod vakuem nesmršťují) | 63/1000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | ISOX63/1000 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 100/250 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | ISOX100/250 |  | 0 | 3 |  |  |  | 0,00 |
| Flange: AISI 304 or AISI 316L or AISI 316Ti | 100/500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | ISOX100/500 |  | 0 | 3 |  |  |  | 0,00 |
| Bellows: AISI 304 or AISI 316L or AISI 316Ti | 100/750 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | ISOX100/750 |  | 0 | 3 |  |  |  | 0,00 |
|  | 100/1000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | ISOX100/1000 |  | 0 | 3 |  |  |  | 0,00 |
|  | 160/250 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | ISOX160/250 |  | 0 | 3 |  |  |  | 0,00 |
|  | 160/500 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | ISOX160/500 |  | 0 | 1 |  |  |  | 0,00 |
|  | 160/750 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | ISOX160/750 |  | 0 | 1 |  |  |  | 0,00 |
|  | 160/1000 |  | Hositrad | Hydraulically Formed Flexible Coupling |  | ISOX160/1000 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Adaptor Flange ISO-K/ISO-F** | 160/63 |  | Hositrad | Addaptor Flange ISO-K/ISO-F |  | ISOA160/63D |  | 0 | 2 |  |  |  | 0,00 |
| **Materiál:** | 160/100 |  | Hositrad | Addaptor Flange ISO-K/ISO-F |  | ISOA160/100D |  | 0 | 1 |  |  |  | 0,00 |
| AISI 304 | 200/100 |  | Hositrad | Addaptor Flange ISO-K/ISO-F |  | ISOA200/100D |  | 0 | 1 |  |  |  | 0,00 |
|  | 200/160 |  | Hositrad | Addaptor Flange ISO-K/ISO-F |  | ISOA200/160D |  | 0 | 1 |  |  |  | 0,00 |
|  | 250/160 |  | Hositrad | Addaptor Flange ISO-K/ISO-F |  | ISOA250/160D |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  | **Celková cena** |  | **28 340,00 €** |
|  |  |  |  |  |  |  |  |  |  |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **CF** | **DN** |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |
|  | **Výrobce** | **Obchodní název** |  | **Objednávací číslo** |  | **Minimální počet [ks]** | **Odhadovaný počet [ks]** |  | **Cen za kus bez DPH** |  | **Celková cena bez DPH** |
| **Komponenty CF dle ISO 3669 a TS/ ISO 3669-2** | |  |  |  |  | [€] |  | [€] |
| **Hexagon Head Screw Set- for Flanges with Through-holes** | 16 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M4x35 - 6Ks Podložka hladká DIN 125 A4 nerez pr.4,3 - 6Ks Matice přesná DIN 934 A4 nerez M4 - 6Ks |  | 1103607017  1702607003  1401607003 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 40 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M6x45 6ks  Podložka hladká DIN 125 A4 nerez pr.6,4 6ks  Matice přesná DIN 934 A4 nerez M6 6ks |  | 1103607053  1702607005  1401607005 |  | 0 | 1 |  |  |  | 0,00 |
| Bolt: AISI 316 or AISI 304 or AISI 316L | 63 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M8x55 - 8ks Podložka hladká DIN 125 A4 nerez pr.8,4 -8ks Matice přesná DIN 934 A4 nerez M8 - 8ks |  | 1103607085  1702607006  1401607007 |  | 0 | 1 |  |  |  | 0,00 |
| Washer: AISI 316 or AISI 304 or AISI 316L | 100 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M8x60 16ks Podložka hladká DIN 125 A4 nerez pr.8,4 16ks Matice přesná DIN 934 A4 nerez M8 16ks |  | 1103607086  1702607006  1401607007 |  | 0 | 1 |  |  |  | 0,00 |
| Nut: AISI 316 or AISI 304 or AISI 316L | 160 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M8x65 20ks  Podložka hladká DIN 125 A4 nerez pr.8,4 20ks  Matice přesná DIN 934 A4 nerez M8 20ks |  | 1103607087  1702607006  1401607007 |  | 0 | 1 |  |  |  | 0,00 |
|  | 200 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M8x70 24ks Podložka hladká DIN 125 A4 nerez pr.8,4 24ks Matice přesná DIN 934 A4 nerez M8 24ks |  | 1103607088  1702607006  1401607007 |  | 0 | 1 |  |  |  | 0,00 |
|  | 250 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M8x70 32ks  Podložka hladká DIN 125 A4 nerez pr.8,4 32ks  Matice přesná DIN 934 A4 nerez M8 32ks |  | 1103607088  1702607006  1401607007 |  | 0 | 1 |  |  |  | 0,00 |
|  | 300 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M10x80 32ks  Podložka hladká DIN 125 A4 nerez pr.10,5 32ks  Matice přesná DIN 934 A4 nerez M10 32ks |  | 1103607120  1702607007  1401607008 |  | 0 | 1 |  |  |  | 0,00 |
|  | 350 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M10x80 36ks  Podložka hladká DIN 125 A4 nerez pr.10,5 36ks Matice přesná DIN 934 A4 nerez M10 36ks |  | 1103607120  1702607007  1401607008 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Hexagon Head Screw Set- for Flanges with Tapped Holes** | 16 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M4x35 6ks Podložka hladká DIN 125 A4 nerez pr.4,3 6ks |  | 1103607017  1702607003 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 40 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M6x45 6ks  Podložka hladká DIN 125 A4 nerez pr.6,4 6ks |  | 1103607053  1702607005 |  | 0 | 1 |  |  |  | 0,00 |
| Bolt: AISI 316 or AISI 304 or AISI 316L | 63 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M8x55 8ks  Podložka hladká DIN 125 A4 nerez pr.8,4 8ks |  | 1103607085  1702607006 |  | 0 | 1 |  |  |  | 0,00 |
| Washer: AISI 316 or AISI 304 or AISI 316L | 100 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M8x60 16ks Podložka hladká DIN 125 A4 nerez pr.8,4 16ks |  | 1103607086  1702607006 |  | 0 | 1 |  |  |  | 0,00 |
|  | 160 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M8x65 20ks  Podložka hladká DIN 125 A4 nerez pr.8,4 20ks |  | 1103607087 1702607006 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Set of Stud Screws with Hexagon Nut** | 40 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M8x55 8ks  Podložka hladká DIN 125 A4 nerez pr.8,4 8ks  Matice přesná DIN 934 A4 nerez M8 8ks |  | 1103607085  1702607006  1401607007 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 63-100 |  | Ingomat | Šroub přesný 02 1103 A4-70 nerez M8x60 16ks  Podložka hladká DIN 125 A4 nerez pr.8,4 16ks  Matice přesná DIN 934 A4 nerez M8 16ks |  | 1103607086  1702607006  1401607007 |  | 0 | 1 |  |  |  | 0,00 |
| Bolt: AISI 316 or AISI 304 or AISI 316L |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Washer: AISI 316 or AISI 304 or AISI 316L |  |  |  |  |  |  |  |  |  |  |  |  |  |
| Nut: AISI 316 or AISI 304 or AISI 316L |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Copper Gasket** | 16 |  | Hositrad | Gaskets Copper - OFHC |  | CG19 |  | 0 | 5 |  |  |  | 0,00 |
| **Materiál:** | 40 |  | Hositrad | Gaskets Copper - OFHC |  | CG40 |  | 0 | 5 |  |  |  | 0,00 |
| Copper OFHC -/2.0040 | 63 |  | Hositrad | Gaskets Copper - OFHC |  | CG64 |  | 0 | 1 |  |  |  | 0,00 |
|  | 100 |  | Hositrad | Gaskets Copper - OFHC |  | CG100 |  | 0 | 1 |  |  |  | 0,00 |
|  | 160 |  | Hositrad | Gaskets Copper - OFHC |  | CG150 |  | 0 | 1 |  |  |  | 0,00 |
|  | 200 |  | Hositrad | Gaskets Copper - OFHC |  | CG200 |  | 0 | 1 |  |  |  | 0,00 |
|  | 250 |  | Hositrad | Gaskets Copper - OFHC |  | CG250 |  | 0 | 1 |  |  |  | 0,00 |
|  | 300 |  | Hositrad | Gaskets Copper - OFHC |  | CG300 |  | 0 | 1 |  |  |  | 0,00 |
|  | 350 |  | Hositrad | Gaskets Copper - OFHC |  | CG350 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Silver-plate Copper Gasket** | 16 |  | Hositrad | Gaskets Copper - Silver Plated |  | CG19SP |  | 0 | 1 |  |  |  | 0,00 |
| NOTE: | 40 |  | Hositrad | Gaskets Copper - Silver Plated |  | CG40SP |  | 0 | 1 |  |  |  | 0,00 |
| Double silver plated | 63 |  | Hositrad | Gaskets Copper - Silver Plated |  | CG64SP |  | 0 | 1 |  |  |  | 0,00 |
|  | 100 |  | Hositrad | Gaskets Copper - Silver Plated |  | CG100SP |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 160 |  | Hositrad | Gaskets Copper - Silver Plated |  | CG150SP |  | 0 | 1 |  |  |  | 0,00 |
| Copper OFHC -/2.0040 | 200 |  | Hositrad | Gaskets Copper - Silver Plated |  | CG200SP |  | 0 | 1 |  |  |  | 0,00 |
|  | 250 |  | Hositrad | Gaskets Copper - Silver Plated |  | CG250SP |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **Elastomer Gasket** | 16 |  | Hositrad | Gaskets Viton |  | VG19 |  | 0 | 1 |  |  |  | 0,00 |
| NOTE: | 40 |  | Hositrad | Gaskets Viton |  | VG38 |  | 0 | 1 |  |  |  | 0,00 |
| Rectangular cross-section | 63 |  | Hositrad | Gaskets Viton |  | VG64 |  | 0 | 1 |  |  |  | 0,00 |
|  | 100 |  | Hositrad | Gaskets Viton |  | VG100 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 160 |  | Hositrad | Gaskets Viton |  | VG150 |  | 0 | 1 |  |  |  | 0,00 |
| Elastomer FPM | 200 |  | Hositrad | Gaskets Viton |  | VG200 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  | **Celková cena** |  | **300,40 €** |
|  |  |  |  |  |  |  |  |  |  |  |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Potrubí** | **L (délka) [mm]** |  | **Výrobce** | **Obchodní název** |  | **Objednávací číslo** |  | **Minimální počet [ks]** | **Odhadovaný počet [ks]** |  | **Cen za kus bez DPH** |  | **Celková cena bez DPH** |
|  |  |  |  | [€] |  | [€] |
| **DN63 ISO-K** | 100 |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=100 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | (101 ÷ 149) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=101-149 |  | 0 | 1 |  |  |  | 0,00 |
| AISI 304 | 150 |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=150 |  | 0 | 1 |  |  |  | 0,00 |
|  | (151 ÷ 249) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=151-249 |  | 0 | 1 |  |  |  | 0,00 |
| **Pozn.:** | 250 |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=250 |  | 0 | 1 |  |  |  | 0,00 |
| Libovolná délka např. v intervalu 101mm až 149mm je značena (101 ÷ 149). | (251 ÷ 499) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=251-499 |  | 0 | 1 |  |  |  | 0,00 |
|  | 500 |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=500 |  | 0 | 1 |  |  |  | 0,00 |
|  | (501 ÷ 749) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=501-749 |  | 0 | 1 |  |  |  | 0,00 |
|  | 750 |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=750 |  | 0 | 1 |  |  |  | 0,00 |
|  | (751 ÷ 999) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=751-999 |  | 0 | 1 |  |  |  | 0,00 |
|  | 1000 |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=1000 |  | 0 | 1 |  |  |  | 0,00 |
|  | (55 ÷ 100) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=55-100 |  | 0 | 1 |  |  |  | 0,00 |
|  | (1001 ÷ 1250) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=1001-1250 |  | 0 | 1 |  |  |  | 0,00 |
|  | (1251 ÷ 1499) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=1251-1499 |  | 0 | 1 |  |  |  | 0,00 |
|  | 1500 |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=1500 |  | 0 | 1 |  |  |  | 0,00 |
|  | (1501 ÷ 1750) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=1501-1750 |  | 0 | 1 |  |  |  | 0,00 |
|  | (1751 ÷ 1999) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=1751-1999 |  | 0 | 1 |  |  |  | 0,00 |
|  | 2000 |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=2000 |  | 0 | 1 |  |  |  | 0,00 |
|  | (2001 ÷ 2250) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=2001-2250 |  | 0 | 1 |  |  |  | 0,00 |
|  | (2251 ÷ 2499) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=2251-2499 |  | 0 | 1 |  |  |  | 0,00 |
|  | 2500 |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=2500 |  | 0 | 1 |  |  |  | 0,00 |
|  | (2501 ÷ 2750) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=2501-2750 |  | 0 | 1 |  |  |  | 0,00 |
|  | (2751 ÷ 2999) |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=2751-2999 |  | 0 | 1 |  |  |  | 0,00 |
|  | 3000 |  | Streicher | Potrubí DN 63 ISO-K |  | DN 63 ISO-K L=3000 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **DN100 ISO-K** | (55 ÷ 100) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=55-100 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 100 |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=100 |  | 0 | 1 |  |  |  | 0,00 |
| AISI 304 | (101 ÷ 249) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=101-249 |  | 0 | 1 |  |  |  | 0,00 |
|  | 250 |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=250 |  | 0 | 1 |  |  |  | 0,00 |
| **Pozn.:** | (251 ÷ 499) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=251-499 |  | 0 | 3 |  |  |  | 0,00 |
| Libovolná délka např. v intervalu 101mm až 249mm je značena (101 ÷ 249). | 500 |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=500 |  | 0 | 2 |  |  |  | 0,00 |
|  | (501 ÷ 749) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=501-749 |  | 0 | 2 |  |  |  | 0,00 |
|  | 750 |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=750 |  | 0 | 1 |  |  |  | 0,00 |
|  | (751 ÷ 999) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=751-999 |  | 0 | 3 |  |  |  | 0,00 |
|  | 1000 |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=1000 |  | 0 | 2 |  |  |  | 0,00 |
|  | (1001 ÷ 1250) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=1001-1250 |  | 0 | 2 |  |  |  | 0,00 |
|  | (1251 ÷ 1499) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=1251-1499 |  | 0 | 2 |  |  |  | 0,00 |
|  | 1500 |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=1500 |  | 0 | 4 |  |  |  | 0,00 |
|  | (1501 ÷ 1750) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=1501-1750 |  | 0 | 2 |  |  |  | 0,00 |
|  | (1751 ÷ 1999) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=1751-1999 |  | 0 | 2 |  |  |  | 0,00 |
|  | 2000 |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=2000 |  | 0 | 3 |  |  |  | 0,00 |
|  | (2001 ÷ 2250) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=2001-2250 |  | 0 | 1 |  |  |  | 0,00 |
|  | (2251 ÷ 2500) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=2251-2500 |  | 0 | 2 |  |  |  | 0,00 |
|  | 2500 |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=2500 |  | 0 | 2 |  |  |  | 0,00 |
|  | (2501 ÷ 2750) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=2501-2750 |  | 0 | 2 |  |  |  | 0,00 |
|  | (2751 ÷ 2999) |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=2751-2999 |  | 0 | 1 |  |  |  | 0,00 |
|  | 3000 |  | Streicher | Potrubí DN 100 ISO-K |  | DN 100 ISO-K L=3000 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| **DN160 ISO-K** | (55 ÷ 100) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=55-100 |  | 0 | 1 |  |  |  | 0,00 |
| **Materiál:** | 100 |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=100 |  | 0 | 1 |  |  |  | 0,00 |
| AISI 304 | (101 ÷ 249) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=101-249 |  | 0 | 1 |  |  |  | 0,00 |
|  | 250 |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=250 |  | 0 | 1 |  |  |  | 0,00 |
| **Pozn.:** | (251 ÷ 499) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=251-499 |  | 0 | 1 |  |  |  | 0,00 |
| Libovolná délka např. v intervalu 101mm až 249mm je značena (101 ÷ 249). | 500 |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=500 |  | 0 | 1 |  |  |  | 0,00 |
|  | (501 ÷ 749) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=501-749 |  | 0 | 1 |  |  |  | 0,00 |
|  | 750 |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=750 |  | 0 | 1 |  |  |  | 0,00 |
|  | (751 ÷ 999) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=751-999 |  | 0 | 1 |  |  |  | 0,00 |
|  | 1000 |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=1000 |  | 0 | 1 |  |  |  | 0,00 |
|  | (1001 ÷ 1250) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=1001-1250 |  | 0 | 1 |  |  |  | 0,00 |
|  | (1251 ÷ 1499) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=1251-1499 |  | 0 | 1 |  |  |  | 0,00 |
|  | 1500 |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=1500 |  | 0 | 1 |  |  |  | 0,00 |
|  | (1501 ÷ 1750) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=1501-1750 |  | 0 | 2 |  |  |  | 0,00 |
|  | (1751 ÷ 1999) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=1751-1999 |  | 0 | 3 |  |  |  | 0,00 |
|  | 2000 |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=2000 |  | 0 | 2 |  |  |  | 0,00 |
|  | (2001 ÷ 2250) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=2001-2250 |  | 0 | 1 |  |  |  | 0,00 |
|  | (2251 ÷ 2500) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=2251-2500 |  | 0 | 1 |  |  |  | 0,00 |
|  | 2500 |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=2500 |  | 0 | 1 |  |  |  | 0,00 |
|  | (2501 ÷ 2750) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=2501-2750 |  | 0 | 1 |  |  |  | 0,00 |
|  | (2751 ÷ 2999) |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=2751-2999 |  | 0 | 1 |  |  |  | 0,00 |
|  | 3000 |  | Streicher | Potrubí DN 160 ISO-K |  | DN 160 ISO-K L=3000 |  | 0 | 1 |  |  |  | 0,00 |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |  | **Celková cena bez DPH** | | |
|  |  |  |  |  |  |  |  |  |  |  | **Potrubí** |  | **39 918,00 €** |