HW - řídící jednotka storage

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| 2078-4H4 | IBM FlashSystem V5100 NVMe Control Enclosure | 1 |
| 9730 | Power Cord - PDU connection | 1 |
| ACBA | SAS Enclosure Attach Card Pair | 1 |
| ACBB | 16Gb FC 4 Port Adapter Pair | 1 |
| ACGE | V5100 64 GB Cache upgrade | 2 |
| ACGX | 120 GB M.2 Boot drive Pair | 1 |
| ACGZ | Manufacturing Indicator #2 | 1 |
| ACSQ | 1m OM3 Fiber Cable (LC) | 4 |
| ACSR | 5m OM3 Fiber Cable (LC) | 4 |
| ADN1 | Order Type 1 - CTO | 1 |
| AET3 | 3.84TB 2.5In NVMe Flash Drive | 12 |
| AG00 | Shipping and Handling NC | 1 |
| AHZE | Hybrid Flash Indicator | 1 |

HW - expanzní jednotka storage

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| 2078-12G | FlashSystem 5100 LFF Expansion Enclosure | 1 |
| 9730 | Power Cord - PDU Connection | 1 |
| AC3E | 14TB 7.2K 3.5 Inch NL HDD | 12 |
| ACUA | 0.6m 12Gb SAS Cable(mSAS HD) | 2 |
| ADN1 | Order Type 1 - CTO | 1 |
| AG00 | Shipping and Handling NC | 1 |
| AHPA | AC Power Supply HE | 1 |
| AHZE | Hybrid Flash Indicator | 1 |

SW - řídící jednotka storage

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| 5639-SDV | 3-Year Registration SWMA for 5639-SV9 | 1 |
| UDX4C5 | Base SW per Device Registration | 1 |
| UDXBC5 | Full Bundle per Device Registration | 2 |
| 5639-SV9 | IBM Spectrum Virtualize Software for FlashSystem 5100 V8 | 1 |
| UDWFC1 | Base SW per Device w/ 1Yr SW Maint | 1 |
| UDWSC1 | Full Bundle per Device w/ 1Yr SW Maint | 2 |

SW - expanzní storage jednotka

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| 5639-SSL | SPECTRUM VIRTUALIZE SOFTWARE FOR STORWIZ | 1 |
| 9000 | BASE PER STORAGE DEVICE SW MAINT 3 YEAR | 1 |
| UCX3C5 | IBM SPECTRUM VIRTUALIZE SOFTWARE FOR STO | 1 |
| 5639-SV8 | IBM Spectrum Virtualize Software for Storwize V50x0 Expansion V8 | 1 |
| UDMUC1 | IBM V50x0 Expansion Base SW with 1 Year SW Maintenance, Per Storage D | 1 |

HW - cache upgrade pro stávající diskové pole IBM v5030

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| 2078-ACHD | V5030 Cache Upgrade | 1 |

HW - SAN

|  |  |  |
| --- | --- | --- |
| **P/N** | **popis** | **ks** |
| 8960-F24 | IBM Storage Networking SAN24B-6 | 2 |
| 2446 | F24 8 x 16Gbps SW SFP Bundle | 2 |
| 7498 | SAN24B-6 8 Port 16Gbps SW Upgrade | 2 |
| AG00 | Shipping and Handling NC | 2 |