**PŘÍLOHA Č. 1 TECHNICKÝ RIDER / STAGEPLAN**

**EXTRA INFO**

Kapela si přiveze vlastní pult BEHRINGER WING a STAGEBOX DL251 Kapela má vlastní inear systém

Kapela má vlastní bezdrátový systém Shure axient – Marpo, Ironkap, Wohnout Kapela si přiveze BACKDROP (12x7m)

Kapela si přiveze FRONTDROP (12x3m) – prosíme o přípravu lanka do výšky 3m od hrany pódia

**CO POTŘEBUJEME ZAJISTIT**

DRUM RISER – 300 x 200 x 40 cm

DJ RISER – 300 x 200 x 40 cm

DJ STŮL – 200 x 100 x 40 cm

MARPO LÁVKA RISER – 600 x 100 x 100 cm – PROSÍME ZAVĚTROVAT PROTI HOUPÁNÍ

2x CAT5 mezi FOH a stage (umístit tak, aby 1x CAT5 vystačila doprostřed pódia) Marcus - Bass amp – Mic stand mid + Mic stand high + Mic Shure SM58 (nebo obdoba) Mika - Kick – Mic stand small

Mika - Hihat – Mic stand mid

Mika - OH – Mic stand high (land stand)

Mika – OH R – Mic stand high + Mic AKG451 (nebo obdoba)

**LINE UP**

|  |  |
| --- | --- |
| **Name** | **Instrument** |
| Marpo | Vocal, Guitar (acoustic), Riser 600x100x100 |
| Ironkap | Vocal |
| Wohnout | Vocal |
| Mika | Riser 300x200x40, OH L, OH R, HH, Kick Stand |
| PartyBoi | Riser 300x200x40, DJ table 200x100x100, Sampler, Laptop, DJ monitor |
| Marcus | Vocal, Bass Guitar (electric), Bass amp, Bass Mic Stand |
| Tomáš | Guitar (electric), Amp, Amp |

**AUX OUTPUTS**

|  |  |
| --- | --- |
| **Name** | **Output** |
| Marpo | Left, Right |
| Ironkap | Left, Right |
| Wohnout | Left, Right |
| Mika | Wedge |
| PartyBoi | Wedge, inear |
| Marcus | Left, Right |
| Tomáš | Left, Right |
| Bass | mono |
|  | Left, Right |

**INPUT**

|  |  |  |
| --- | --- | --- |
| **Channel** | **Name** | **Instrument** |
| 1 | Mika | Kick in |
| 2 | Mika | Kick out |
| 3 | Mika | Snare Top |
| 4 | Mika | Snare Bottom |
| 5 | Mika | Hi Hat |
| 6 | Mika | Tom 1 |
| 7 | Mika | Tom 2 |
| 8 | Mika | Tom 3 |
| 9 | Mika | Floor Tom |
| 10 | Mika | OH L |
| 11 | Mika | OH R |
| 12 | Marcus | Bass line |
| 13 | Marcus | Bass mic |
| 14 | Marpo | Guitar Marpo |
| 15 | Tomáš | Guitar Tom L |
| 16 | Tomáš | Guitar Tom R |
| 17 | Partyboi | DJ L |
| 18 | Partyboi | DJ R |
| 19 | Partyboi | DJ Bass |
| 20 | Partyboi | Click |
| 21 | Partyboi | Guit L |
| 22 | Partyboi | Guit R |
| 23 | Partyboi | VOX L |
| 24 | Partyboi | VOX R |
| 25 | Partyboi | KEY L |
| 26 | Partyboi | KEY R |
| 27 | Partyboi | DJ intro |
| 28 | Partyboi | DJ intro |
| 29 | Marcus | Vox |
| 30 | Ironkap | Vox |
| 31 | Marpo | Vox |
| 32 | Wohnout | Vox |


**MONITOR GROUPS**

|  |  |
| --- | --- |
| **Group** | **Soundmix** |
| Group 1 | DJ Monitor |




























**SFX EFEKTY**

Kapela si přiveze SFX efekty dle dohody s pořadatelem. POŘADATEL ZAJIŠŤUJE TLAKOVÉ LAHVE (CO2, PB) NA SVÉ NÁKLADY!!! Požadovaný počet tlakových lahví bude upřesněn dle dohody mezi managerem kapely a pořadatelem akce.

# STAGEPLAN MARPO & TROUBLEGANG



**BACK**



# STAGE 10x8m

**RISER / NIVTEC 600x100x100**

**SANDWICH NEBO ZAVĚTROVAT!!!**

**RISER 300x200x40**

**RISER 300x200x40**

Monitor (1)


PartyBoi

Mika

**DJ STŮL 200x100x100**

Sampler

Bass Amp

Amp Amp

in-ear (1)

Kick Stand

Bass Mic Stand

Tomáš

Ironkap Wohnout Marcus

Guitar (electric)

Vocal

Marpo

Vocal

Bass Guitar (electric)

Vocal

Mic (vocals)

**kontakt zvuk: Michal Kazda,** [**Michal-Kazda@seznam.cz,**](mailto:Michal-Kazda@seznam.cz) **+420 777 841 583**

**kontakt technika: Vlasta Kastl,** [**vlasta.kastl@gmail.com,**](mailto:vlasta.kastl@gmail.com) **+420 776 212 289**

**FRONT**