Lokální dodavatel techniky zajistí:
-	PA systém odpovídajícího výkonu pro pokrytí celého auditoria
-	3 ks dvoupásmových odposlechových boxů a 1 ks třípásmový drum fill
-	Akceptovatelné značky ozvučení PA a odposlechů: L-Acoustics, Adamson, d+b, Nexo
-	4 ks (min. 2 ks) koaxiální kabely 75 ohm s konektory BNC natažené mezi pódiem a FOH
-	1 ks riser 3 x 2 x 0,4 m plus 1 x riser 2 x 2 x 0,4 m dle stageplánu + 2 x 2 x 0,2 m (pod klávesy pokud to rozměry pódia umožní) - Kompletní set mikrofonů, Dl boxů, stativů a kabelů dle input listu
Kapela si veze vlastní pult Digico SD8 včetně MADI rack, 4 ks IEM a bezdrátový mikrofon.
Frekvenční pásmo IEM 530-660 MHz
Frekvenční pásmo mikrofonu 470-534 MHz
Pro open air akce je třeba zajistit kvalitně zastřešený prostor FOH min 150 x 200 cm.
Dlouhé XLR natáhnout mezi piáno a bicí Piano -> Drums

Input list
Channel	Band Member	Instrument	Mic / DI	Insert	Stand	
1	Jarda - Drums	Kick	Mic	Vlastní	Mal stojan	
2	Jarda - Drums	Snare Top	Mic	Vlastní		
3	Jarda - Drums	Snare Bottom	Mic	Vlastní		
4	Jarda - Drums	Hi Hat	Mic	Vlastní	Střední stojan	
5	Jarda - Drums	Ride	Mic	Vlastní		
6	Jarda - Drums	Tom 2	Mic	Vlastní		
7	Jarda - Drums	Floor Tom 1	Mic	Vlastní		
8	Jarda - Drums	Overhead L	Mic	Vlastní	Boom stojan	
9	Jarda - Drums	Overhead R	Mic	Vlastní	Boom stojan	
10	Víťa - Percussions	Bonga	Mic	Shure SM57		
11	Víťa - Percussions	Conga 1	Mic	Shure SM57		
12	Víťa - Percussions	Conga 2	Mic	Shure SM57		
13	Víťa - Percussions	Djembe Bass	Mic	Beta 52	Mal stojan	
14	Víťa - Percussions	Djembe Top	Mic	Shure SM57	Boom stojan	
15	Víťa - Percussions	Overhead L	Mic	AKG C451	Boom stojan	
16	Víťa - Percussions	Overhead R	Mic	AKG C451	Boom stojan	
17	Vašek - Bass Guitar	Bass Guitar	Line XLR	Amp XLR		
18	Jirka - Guitar Right	El. Guitar Right	Mic	Sen e906	Mal stojan	
19	Jirka - Guitar Right	AC. Guitar Right	Line XLR	AER Combo		
20	Petr - Guitar Left	El. Guitar Left	Mic	Sen e906	Mal stojan	
21	Petr - Guitar Left	El. Guitar Left 2	Line XLR	Amp XLR		
22	Pája - Piano	AC. Guitar	DI Box			
23	Pája - Piano	Piano L	XLR	Piano XLR Out		
24	Pája - Piano	Piano R	XLR	Piano XLR Out		
25	Pája - Piano	Sampler L	DI Box	Jack Mono		
26	Pája - Piano	Sampler R	DI Box	Jack Mono		
27	Pája - Piano	VOC	Mic	Vlastní	Boom stojan	
28	Jirka - Guitar Right	VOC	Mic	Shure SM58	Boom stojan	
29	Anna K - Main Vocal	VOC	Wireless Mic	Vlastní	Boom stojan	
30	Vašek - Bass Guitar	VOC	Mic	Shure SM58	Boom stojan	
31	Petr - Guitar Left	VOC	Mic	Shure SM58	Boom stojan	
32	Jarda - Drums	Kick	Mic	Vlastní		
39.	SPD L (Percussion)		DI Box			
40.	SPD R (Percussion)		DI Box			

Monitor
AUX Out	Location	
AUX 1	IEM wireless	Jirka - Guitar right	
AUX 2	2x Wedge	AK - Main Vocal	
AUX 3	1x Wedge	Vašek - Bass Guitar	
AUX 4	IEM wire	Petr - Guitar Left - natahuje se kabelem XLR ke kytaristovi	
AUX 5		Prázdná!!!	
AUX 6	1x Drum fill	Jarda - Drumfill	
AUX 7	IEM Stagebox	Pája - Piano	
AUX 8	IEM Stagebox	AK - Main Vocal	
AUX 9	IEM Drum Riser	Jarda - Drums - natahuje se kabelem XLR k bicím	
AUX 10	IEM Perc. Riser	Víťa - Percussion - natahuje se kabelem XLR k perkusím	
AUX 11	IEM Perc. Riser	Víťa - Percussion - natahuje se kabelem XLR k perkusím	
AUX 12	IEM Stagebox	Technik